`verilator_config

// Unnamed blocks do not influence logic
lint_off -rule GENUNNAMED

// Unconnected IC memory output pins
lint_off -rule PINCONNECTEMPTY -file "*/el2_ifu_ic_mem.sv"

// These require revisit to remove multiple definitions of variables with same names
lint_off -rule VARHIDDEN -file "*/axi4_to_ahb.sv"
lint_off -rule VARHIDDEN -file "*/el2_ifu_bp_ctl.sv"
lint_off -rule VARHIDDEN -file "*/el2_ifu_mem_ctl.sv"
lint_off -rule VARHIDDEN -file "*/el2_exu_alu_ctl.sv"
lint_off -rule VARHIDDEN -file "*/el2_pic_ctrl.sv"
lint_off -rule VARHIDDEN -file "*/el2_veer_lockstep.sv"

// Width related warning require explicit type casting
lint_off -rule WIDTHTRUNC -file "*/ahb_to_axi4.sv"
lint_off -rule WIDTHTRUNC -file "*/axi4_to_ahb.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dma_ctrl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_ifu_ifc_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_ifu_bp_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_ifu_aln_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dec_decode_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dec_ib_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dec_tlu_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dec_trigger.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lib.sv"
lint_off -rule WIDTHTRUNC -file "*/beh_lib.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lsu_bus_buffer.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dec_pmp_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lsu_addrcheck.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lsu_dccm_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lsu_dccm_mem.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_lsu_trigger.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_ifu_iccm_mem.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_ifu_mem_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_exu.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_exu_alu_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_exu_div_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_exu_mul_ctl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_dbg.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_pic_ctrl.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_pmp.sv"
lint_off -rule WIDTHTRUNC -file "*/el2_mem_if.sv"

lint_off -rule WIDTHEXPAND -file "*/el2_exu.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_pic_ctrl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_ifu_bp_ctl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_ifu_mem_ctl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_ifu_iccm_mem.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_lsu_addrcheck.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_lsu_bus_buffer.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_lsu_stbuf.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_lsu_dccm_ctl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_lsu_dccm_mem.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_exu_mul_ctl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_dec_tlu_ctl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_dma_ctrl.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_dbg.sv"
lint_off -rule WIDTHEXPAND -file "*/el2_veer_lockstep.sv" -lines 391

// Unused parameters are probably safe to remove from RTL
lint_off -rule UNUSEDPARAM -file "*/axi4_to_ahb.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_ifu.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_pic_ctrl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_dma_ctrl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_ifu_bp_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_ifu_mem_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_dec_tlu_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_lsu_dccm_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_lsu_dccm_mem.sv"

// Gated clock, expected latch
lint_off -rule LATCH -file "*/beh_lib.sv" -lines 781

lint_off -rule BLKSEQ -file "*/beh_lib.sv" -lines 783

// The Verilator reports that `core_rst_l` is being used in sync and async nets,
// pointing to `rvdff` module as a source of the problem. Since the `rvdff` looks
// unrelated to `core_rst_l`, it requires a closer investigation.
lint_off -rule SYNCASYNCNET -file "*/el2_veer.sv" -lines 41

// Unused clocks from shadow core
lint_off -rule PINCONNECTEMPTY -file "*/el2_veer_lockstep.sv" -lines 830-831

// Logic that might be not optimal for event based model used by Verilator
lint_off -rule UNOPTFLAT -file "*/axi4_to_ahb.sv"
lint_off -rule UNOPTFLAT -file "*/el2_ifu_ifc_ctl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_dec_decode_ctl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_exu_mul_ctl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_exu_div_ctl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_lsu.sv"
lint_off -rule UNOPTFLAT -file "*/el2_lsu_lsc_ctl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_pic_ctrl.sv"
lint_off -rule UNOPTFLAT -file "*/el2_lsu_bus_buffer.sv"

// Warnings related to the generated `el2_param.vh`
lint_off -rule UNUSEDPARAM -file "*/el2_ifu_compress_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_dec_gpr_ctl.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_dec_trigger.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_lsu_trigger.sv"
lint_off -rule UNUSEDPARAM -file "*/el2_lsu_clkdomain.sv"

lint_off -rule WIDTHTRUNC -file "*/el2_ifu_compress_ctl.sv"
