<?xml version='1.0' encoding='UTF-8'?>
<Project NoOfControllers="1" >
    <ModuleName>mig_37</ModuleName>
    <dci_inouts_inputs>1</dci_inouts_inputs>
    <dci_outputs>0</dci_outputs>
    <Debug_En>ON</Debug_En>
    <TargetFPGA>xc6vlx240t-ff1156/-1</TargetFPGA>
    <Version>3.7</Version>
    <SystemClock>Differential</SystemClock>
    <PinSelectionFlag>FALSE</PinSelectionFlag>
    <IODelayHighPerformanceMode>HIGH</IODelayHighPerformanceMode>
    <InternalVref>0</InternalVref>
    <Controller number="0" >
        <MemoryDevice>DDR3_SDRAM/SODIMMs/MT4JSF6464HY-1G1</MemoryDevice>
        <TimePeriod>2500</TimePeriod>
        <DataWidth>64</DataWidth>
        <DeepMemory>1</DeepMemory>
        <DataMask>1</DataMask>
        <CustomPart>FALSE</CustomPart>
        <NewPartName/>
        <RowAddress>13</RowAddress>
        <ColAddress>10</ColAddress>
        <BankAddress>3</BankAddress>
        <MasterBanks>25</MasterBanks>
        <TimingParameters>
            <Parameters twtr="7.5" trrd="7.5" trefi="7.8" tfaw="45" trtp="7.5" trfc="110" trp="13.13" tras="37.5" trcd="13.13" />
        </TimingParameters>
        <ECC>Disabled</ECC>
        <DiscreteBankSelections>1</DiscreteBankSelections>
        <CaptureClock>36</CaptureClock>
        <UserMemoryAddressMap>ROW_BANK_COLUMN</UserMemoryAddressMap>
        <Ordering>Strict</Ordering>
        <BankSelection>
            <Bank SysClk="0" Data="1" name="25" Address="0" wasso="40" />
            <Bank SysClk="0" Data="1" name="26" Address="0" wasso="40" />
            <Bank SysClk="1" Data="0" name="34" Address="0" wasso="40" />
            <Bank SysClk="0" Data="1" name="35" Address="0" wasso="40" />
            <Bank SysClk="0" Data="0" name="36" Address="1" wasso="40" />
        </BankSelection>
        <mrBurstLength name="Burst Length" >8 - Fixed</mrBurstLength>
        <mrBurstType name="Read Burst Type" >Sequential</mrBurstType>
        <mrCasLatency name="CAS Latency" >6</mrCasLatency>
        <mrMode name="Mode" >Normal</mrMode>
        <mrDllReset name="DLL Reset" >No</mrDllReset>
        <mrPdMode name="DLL control for precharge PD" >Slow Exit</mrPdMode>
        <emrDllEnable name="DLL Enable" >Enable</emrDllEnable>
        <emrOutputDriveStrength name="Output Driver Impedance Control" >RZQ/7</emrOutputDriveStrength>
        <emrRTT name="RTT (nominal) - On Die Termination (ODT)" >RZQ/4</emrRTT>
        <emrPosted name="Additive Latency (AL)" >0</emrPosted>
        <emrOCD name="Write Leveling Enable" >Disabled</emrOCD>
        <emrDQS name="TDQS enable" >Enabled</emrDQS>
        <emrRDQS name="Qoff" >Output Buffer Enabled</emrRDQS>
        <mr2PartialArraySelfRefresh name="Partial-Array Self Refresh" >Full Array</mr2PartialArraySelfRefresh>
        <mr2CasWriteLatency name="CAS write latency" >5</mr2CasWriteLatency>
        <mr2AutoSelfRefresh name="Auto Self Refresh" >Enabled</mr2AutoSelfRefresh>
        <mr2SelfRefreshTempRange name="High Temparature Self Refresh Rate" >Normal</mr2SelfRefreshTempRange>
        <mr2RTTWR name="RTT_WR - Dynamic On Die Termination (ODT)" >Dynamic ODT off</mr2RTTWR>
        <PortInterface>NATIVE</PortInterface>
    </Controller>
</Project>
