# Copyright (C) 1991-2006 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.


# The default values for assignments are stored in the file
#		full_featured_assignment_defaults.qdf
# If this file doesn't exist, and for assignments not listed, see file
#		assignment_defaults.qdf

# Altera recommends that you do not modify this file. This
# file is updated automatically by the Quartus II software
# and any changes you make may be lost or overwritten.


set_global_assignment -name FAMILY "Stratix II"
set_global_assignment -name DEVICE EP2S60F672C3
#set_global_assignment -name TOP_LEVEL_ENTITY full_featured
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 6.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "12:54:53  MAY 22, 2006"
set_global_assignment -name LAST_QUARTUS_VERSION "6.0 SP1"
#set_global_assignment -name DEVICE_FILTER_PACKAGE FBGA
#set_global_assignment -name DEVICE_FILTER_PIN_COUNT 672
#set_global_assignment -name DEVICE_FILTER_SPEED_GRADE FASTEST
#set_global_assignment -name BDF_FILE full_featured.bdf
#set_global_assignment -name POST_FLOW_SCRIPT_FILE "quartus_sh:auto_verify_ddr_timing.tcl"
set_global_assignment -name NUM_PARALLEL_PROCESSORS 2
set_global_assignment -name EDA_SIMULATION_TOOL "ModelSim (VHDL output from Quartus II)"

set_location_assignment PIN_U25 -to address[2]
set_location_assignment PIN_T25 -to address[3]
set_location_assignment PIN_T24 -to address[4]
set_location_assignment PIN_V20 -to address[5]
set_location_assignment PIN_V19 -to address[6]
set_location_assignment PIN_U20 -to address[7]
set_location_assignment PIN_U19 -to address[8]
set_location_assignment PIN_T22 -to address[9]
set_location_assignment PIN_T21 -to address[10]
set_location_assignment PIN_T20 -to address[11]
set_location_assignment PIN_T19 -to address[12]
set_location_assignment PIN_U22 -to address[13]
set_location_assignment PIN_U21 -to address[14]
set_location_assignment PIN_V22 -to address[15]
set_location_assignment PIN_Y24 -to eth_nbe[0] #byteenablen_to_the_lan91c111[0]
set_location_assignment PIN_Y23 -to eth_nbe[1] #byteenablen_to_the_lan91c111[1]
set_location_assignment PIN_AA24 -to eth_nbe[2] #byteenablen_to_the_lan91c111[2]
set_location_assignment PIN_AA23 -to eth_nbe[3] #byteenablen_to_the_lan91c111[3]
#little endian encoding of data bus
set_location_assignment PIN_D15 -to data[24] #ext_flash_enet_bus_data[0]
set_location_assignment PIN_G15 -to data[25] #ext_flash_enet_bus_data[1]
set_location_assignment PIN_E19 -to data[26] #ext_flash_enet_bus_data[2]
set_location_assignment PIN_D20 -to data[27] #ext_flash_enet_bus_data[3]
set_location_assignment PIN_G19 -to data[28] #ext_flash_enet_bus_data[4]
set_location_assignment PIN_D19 -to data[29] #ext_flash_enet_bus_data[5]
set_location_assignment PIN_E20 -to data[30] #ext_flash_enet_bus_data[6]
set_location_assignment PIN_F20 -to data[31] #ext_flash_enet_bus_data[7]
set_location_assignment PIN_M20 -to data[16] #ext_flash_enet_bus_data[8]
set_location_assignment PIN_M19 -to data[17] #ext_flash_enet_bus_data[9]
set_location_assignment PIN_N20 -to data[18] #ext_flash_enet_bus_data[10]
set_location_assignment PIN_N19 -to data[19] #ext_flash_enet_bus_data[11]
set_location_assignment PIN_N22 -to data[20] #ext_flash_enet_bus_data[12]
set_location_assignment PIN_N21 -to data[21] #ext_flash_enet_bus_data[13]
set_location_assignment PIN_M22 -to data[22] #ext_flash_enet_bus_data[14]
set_location_assignment PIN_M21 -to data[23] #ext_flash_enet_bus_data[15]
set_location_assignment PIN_M24 -to data[8] #ext_flash_enet_bus_data[16]
set_location_assignment PIN_M23 -to data[9] #ext_flash_enet_bus_data[17]
set_location_assignment PIN_L19 -to data[10] #ext_flash_enet_bus_data[18]
set_location_assignment PIN_L18 -to data[11] #ext_flash_enet_bus_data[19]
set_location_assignment PIN_L21 -to data[12] #ext_flash_enet_bus_data[20]
set_location_assignment PIN_L20 -to data[13] #ext_flash_enet_bus_data[21]
set_location_assignment PIN_L23 -to data[14] #ext_flash_enet_bus_data[22]
set_location_assignment PIN_L22 -to data[15] #ext_flash_enet_bus_data[23]
set_location_assignment PIN_K20 -to data[0] #ext_flash_enet_bus_data[24]
set_location_assignment PIN_K19 -to data[1] #ext_flash_enet_bus_data[25]
set_location_assignment PIN_K22 -to data[2] #ext_flash_enet_bus_data[26]
set_location_assignment PIN_K21 -to data[3] #ext_flash_enet_bus_data[27]
set_location_assignment PIN_J20 -to data[4] #ext_flash_enet_bus_data[28]
set_location_assignment PIN_J19 -to data[5] #ext_flash_enet_bus_data[29]
set_location_assignment PIN_J22 -to data[6] #ext_flash_enet_bus_data[30]
set_location_assignment PIN_J21 -to data[7] #ext_flash_enet_bus_data[31]
set_location_assignment PIN_W23 -to gpio[4] #irq_from_the_lan91c111
set_location_assignment PIN_AD26 -to rxd1 #rxd_to_the_uart1
set_location_assignment PIN_AB23 -to txd1 #txd_from_the_uart1
set_location_assignment PIN_W15 -to errorn   #out_port_from_the_led_pio[0]
set_location_assignment PIN_V14 -to gpio[1] #out_port_from_the_led_pio[1]
set_location_assignment PIN_AD17 -to gpio[2] #out_port_from_the_led_pio[2]
set_location_assignment PIN_AA17 -to gpio[3] #out_port_from_the_led_pio[3]
set_location_assignment PIN_V16 -to dsuact   #out_port_from_the_led_pio[4]
set_location_assignment PIN_AB17 -to gpio[5] #out_port_from_the_led_pio[5]
set_location_assignment PIN_AD18 -to gpio[6] #out_port_from_the_led_pio[6]
set_location_assignment PIN_V17 -to gpio[7] #out_port_from_the_led_pio[7]
set_location_assignment PIN_P4 -to gpio[8] #in_port_to_the_button_pio[0]
set_location_assignment PIN_P5 -to gpio[9] #in_port_to_the_button_pio[1]
set_location_assignment PIN_N6 -to gpio[10] #in_port_to_the_button_pio[2]
set_location_assignment PIN_N7 -to dsubren  #in_port_to_the_button_pio[3]
set_location_assignment PIN_M2 -to LCD_E_from_the_lcd_display
set_location_assignment PIN_L3 -to LCD_RS_from_the_lcd_display
set_location_assignment PIN_M1 -to LCD_RW_from_the_lcd_display
set_location_assignment PIN_G6 -to LCD_data_to_and_from_the_lcd_display[0]
set_location_assignment PIN_G7 -to LCD_data_to_and_from_the_lcd_display[1]
set_location_assignment PIN_H5 -to LCD_data_to_and_from_the_lcd_display[2]
set_location_assignment PIN_H6 -to LCD_data_to_and_from_the_lcd_display[3]
set_location_assignment PIN_J5 -to LCD_data_to_and_from_the_lcd_display[4]
set_location_assignment PIN_J6 -to LCD_data_to_and_from_the_lcd_display[5]
set_location_assignment PIN_H7 -to LCD_data_to_and_from_the_lcd_display[6]
set_location_assignment PIN_H8 -to LCD_data_to_and_from_the_lcd_display[7]
set_location_assignment PIN_V25 -to address[0]
set_location_assignment PIN_U26 -to address[1]
set_location_assignment PIN_V21 -to address[16]
set_location_assignment PIN_W22 -to address[17]
set_location_assignment PIN_W21 -to address[18]
set_location_assignment PIN_V24 -to address[19]
set_location_assignment PIN_V23 -to address[20]
set_location_assignment PIN_U24 -to address[21]
set_location_assignment PIN_U23 -to address[22]
set_location_assignment PIN_R24 -to address[23]
set_location_assignment PIN_H20 -to oen #read_n_to_the_ext_flash
set_location_assignment PIN_H19 -to romsn #select_n_to_the_ext_flash
set_location_assignment PIN_V26 -to writen #write_n_to_the_ext_flash
set_location_assignment PIN_K18 -to byten  #byte_n_to_the_ext_flash
set_location_assignment PIN_H22 -to wpn    #wp_n_to_the_ext_flash
set_location_assignment PIN_G16 -to ssaddr[2] #address_to_the_ext_ssram[2] 
set_location_assignment PIN_G17 -to ssaddr[3] #address_to_the_ext_ssram[3] 
set_location_assignment PIN_E26 -to ssaddr[4] #address_to_the_ext_ssram[4] 
set_location_assignment PIN_E25 -to ssaddr[5] #address_to_the_ext_ssram[5] 
set_location_assignment PIN_E24 -to ssaddr[6] #address_to_the_ext_ssram[6] 
set_location_assignment PIN_E23 -to ssaddr[7] #address_to_the_ext_ssram[7] 
set_location_assignment PIN_F26 -to ssaddr[8] #address_to_the_ext_ssram[8] 
set_location_assignment PIN_F25 -to ssaddr[9] #address_to_the_ext_ssram[9] 
set_location_assignment PIN_C17 -to ssaddr[10] #address_to_the_ext_ssram[10] 
set_location_assignment PIN_C18 -to ssaddr[11] #address_to_the_ext_ssram[11] 
set_location_assignment PIN_C19 -to ssaddr[12] #address_to_the_ext_ssram[12] 
set_location_assignment PIN_C20 -to ssaddr[13] #address_to_the_ext_ssram[13] 
set_location_assignment PIN_G26 -to ssaddr[14] #address_to_the_ext_ssram[14] 
set_location_assignment PIN_G25 -to ssaddr[15] #address_to_the_ext_ssram[15] 
set_location_assignment PIN_G24 -to ssaddr[16] #address_to_the_ext_ssram[16] 
set_location_assignment PIN_G23 -to ssaddr[17] #address_to_the_ext_ssram[17] 
set_location_assignment PIN_G21 -to ssaddr[18] #address_to_the_ext_ssram[18] 
set_location_assignment PIN_G20 -to ssaddr[19] #address_to_the_ext_ssram[19] 
set_location_assignment PIN_H26 -to ssaddr[20] #address_to_the_ext_ssram[20]
set_location_assignment PIN_B16 -to ssram_adscn #adsc_n_to_the_ext_ssram
set_location_assignment PIN_H23 -to ssram_bw[0] #bw_n_to_the_ext_ssram[0]
set_location_assignment PIN_J23 -to ssram_bw[1] #bw_n_to_the_ext_ssram[1]
set_location_assignment PIN_K24 -to ssram_bw[2] #bw_n_to_the_ext_ssram[2]
set_location_assignment PIN_F16 -to ssram_bw[3] #bw_n_to_the_ext_ssram[3]
set_location_assignment PIN_F17 -to ssram_wen #bwe_n_to_the_ext_ssram
set_location_assignment PIN_C16 -to ssram_ce1n #chipenable1_n_to_the_ext_ssram
set_location_assignment PIN_L25 -to ssram_ce2 #chipenable2_to_the_ext_ssram
set_location_assignment PIN_L24 -to ssram_ce3n #chipenable3_n_to_the_ext_ssram
set_location_assignment PIN_A17 -to ssdata[0] #data_to_and_from_the_ext_ssram[0]
set_location_assignment PIN_A18 -to ssdata[1] #data_to_and_from_the_ext_ssram[1]
set_location_assignment PIN_A19 -to ssdata[2] #data_to_and_from_the_ext_ssram[2]
set_location_assignment PIN_A20 -to ssdata[3] #data_to_and_from_the_ext_ssram[3]
set_location_assignment PIN_B17 -to ssdata[4] #data_to_and_from_the_ext_ssram[4]
set_location_assignment PIN_B18 -to ssdata[5] #data_to_and_from_the_ext_ssram[5]
set_location_assignment PIN_B19 -to ssdata[6] #data_to_and_from_the_ext_ssram[6]
set_location_assignment PIN_B20 -to ssdata[7] #data_to_and_from_the_ext_ssram[7]
set_location_assignment PIN_B24 -to ssdata[8] #data_to_and_from_the_ext_ssram[8]
set_location_assignment PIN_C22 -to ssdata[9] #data_to_and_from_the_ext_ssram[9]
set_location_assignment PIN_B22 -to ssdata[10] #data_to_and_from_the_ext_ssram[10]
set_location_assignment PIN_C21 -to ssdata[11] #data_to_and_from_the_ext_ssram[11]
set_location_assignment PIN_E18 -to ssdata[12] #data_to_and_from_the_ext_ssram[12]
set_location_assignment PIN_D18 -to ssdata[13] #data_to_and_from_the_ext_ssram[13]
set_location_assignment PIN_E17 -to ssdata[14] #data_to_and_from_the_ext_ssram[14]
set_location_assignment PIN_D17 -to ssdata[15] #data_to_and_from_the_ext_ssram[15]
set_location_assignment PIN_F23 -to ssdata[16] #data_to_and_from_the_ext_ssram[16]
set_location_assignment PIN_F22 -to ssdata[17] #data_to_and_from_the_ext_ssram[17]
set_location_assignment PIN_F21 -to ssdata[18] #data_to_and_from_the_ext_ssram[18]
set_location_assignment PIN_B23 -to ssdata[19] #data_to_and_from_the_ext_ssram[19]
set_location_assignment PIN_D25 -to ssdata[20] #data_to_and_from_the_ext_ssram[20]
set_location_assignment PIN_F24 -to ssdata[21] #data_to_and_from_the_ext_ssram[21]
set_location_assignment PIN_H21 -to ssdata[22] #data_to_and_from_the_ext_ssram[22]
set_location_assignment PIN_F19 -to ssdata[23] #data_to_and_from_the_ext_ssram[23]
set_location_assignment PIN_B21 -to ssdata[24] #data_to_and_from_the_ext_ssram[24]
set_location_assignment PIN_A21 -to ssdata[25] #data_to_and_from_the_ext_ssram[25]
set_location_assignment PIN_A22 -to ssdata[26] #data_to_and_from_the_ext_ssram[26]
set_location_assignment PIN_A24 -to ssdata[27] #data_to_and_from_the_ext_ssram[27]
set_location_assignment PIN_C26 -to ssdata[28] #data_to_and_from_the_ext_ssram[28]
set_location_assignment PIN_C25 -to ssdata[29] #data_to_and_from_the_ext_ssram[29]
set_location_assignment PIN_D24 -to ssdata[30] #data_to_and_from_the_ext_ssram[30]
set_location_assignment PIN_C23 -to ssdata[31] #data_to_and_from_the_ext_ssram[31]
set_location_assignment PIN_J26 -to ssram_oen #outputenable_n_to_the_ext_ssram
set_location_assignment PIN_N4 -to gpio[16] #out_port_from_the_seven_seg_pio[0]
set_location_assignment PIN_M6 -to gpio[17] #out_port_from_the_seven_seg_pio[1]
set_location_assignment PIN_M5 -to gpio[18] #out_port_from_the_seven_seg_pio[2]
set_location_assignment PIN_M8 -to gpio[19] #out_port_from_the_seven_seg_pio[3]
set_location_assignment PIN_M7 -to gpio[20] #out_port_from_the_seven_seg_pio[4]
set_location_assignment PIN_L9 -to gpio[21] #out_port_from_the_seven_seg_pio[5]
set_location_assignment PIN_L8 -to gpio[22] #out_port_from_the_seven_seg_pio[6]
set_location_assignment PIN_N5 -to gpio[23] #out_port_from_the_seven_seg_pio[7]
set_location_assignment PIN_L6 -to gpio[24] #out_port_from_the_seven_seg_pio[8]
set_location_assignment PIN_M4 -to gpio[25] #out_port_from_the_seven_seg_pio[9]
set_location_assignment PIN_M3 -to gpio[26] #out_port_from_the_seven_seg_pio[10]
set_location_assignment PIN_L5 -to gpio[27] #out_port_from_the_seven_seg_pio[11]
set_location_assignment PIN_L4 -to gpio[28] #out_port_from_the_seven_seg_pio[12]
set_location_assignment PIN_K9 -to gpio[29] #out_port_from_the_seven_seg_pio[13]
set_location_assignment PIN_K8 -to gpio[30] #out_port_from_the_seven_seg_pio[14]
set_location_assignment PIN_L7 -to gpio[31] #out_port_from_the_seven_seg_pio[15]
set_location_assignment PIN_B13 -to ddr_clkin #osc_clk0
set_location_assignment PIN_P25  -to clk #osc_clk1
set_location_assignment PIN_AA15 -to resetn #pld_clear_n
set_location_assignment PIN_C3 -to ddr_clk #clk_to_sdram[0]
set_location_assignment PIN_C4 -to ddr_clkn #clk_to_sdram_n[0]
set_location_assignment PIN_B10 -to ddr_ad[0]
set_location_assignment PIN_B9 -to ddr_ad[1]
set_location_assignment PIN_B8 -to ddr_ad[2]
set_location_assignment PIN_B6 -to ddr_ad[3]
set_location_assignment PIN_C5 -to ddr_ad[4]
set_location_assignment PIN_E11 -to ddr_ad[5]
set_location_assignment PIN_E10 -to ddr_ad[6]
set_location_assignment PIN_E9 -to ddr_ad[7]
set_location_assignment PIN_E8 -to ddr_ad[8]
set_location_assignment PIN_E7 -to ddr_ad[9]
set_location_assignment PIN_F11 -to ddr_ad[10]
set_location_assignment PIN_F10 -to ddr_ad[11]
set_location_assignment PIN_F8 -to ddr_ad[12]
set_location_assignment PIN_G10 -to ddr_ba[0]
set_location_assignment PIN_G11 -to ddr_ba[1]
set_location_assignment PIN_B3 -to ddr_casb
set_location_assignment PIN_F13 -to ddr_cke
set_location_assignment PIN_E12 -to ddr_csb
set_location_assignment PIN_A3 -to ddr_rasb
set_location_assignment PIN_B4 -to ddr_web
set_location_assignment PIN_A12 -to ssram_clk
set_location_assignment PIN_AA22 -to eth_nads #enet_ads_n
set_location_assignment PIN_AB25 -to eth_aen
set_location_assignment PIN_Y26 -to eth_readn #ior_n_to_the_lan91c111
set_location_assignment PIN_Y25 -to eth_writen #iow_n_to_the_lan91c111

set_location_assignment PIN_AA21 -to eth_lclk #ENET_LCLK
#set_location_assignment PIN_Y7 -to eth_ldevn #ENET_LDEV_N
set_location_assignment PIN_W26 -to eth_nrdyrtn #ENET_RDYRTN_N
#set_location_assignment PIN_W20 -to eth_srdyn #ENET_SRDY_N
set_location_assignment PIN_W19 -to eth_nvlbus #ENET_VLBUS_N
set_location_assignment PIN_AA25 -to eth_wnr #ENET_W_R_N
set_location_assignment PIN_Y24 -to eth_nbe[0] #byteenablen_to_the_lan91c111[0]
set_location_assignment PIN_Y23 -to eth_nbe[1] #byteenablen_to_the_lan91c111[1]
set_location_assignment PIN_AA24 -to eth_nbe[2] #byteenablen_to_the_lan91c111[2]
set_location_assignment PIN_AA23 -to eth_nbe[3] #byteenablen_to_the_lan91c111[3]
set_location_assignment PIN_AA26 -to eth_ncycle #ENET_CYCLE_N
set_location_assignment PIN_W24 -to eth_ndatacs #ENET_DATACS_N

set_location_assignment PIN_AB11 -to cf_detect
set_location_assignment PIN_K3  -to ata_intrq
set_location_assignment PIN_G2 -to ata_iordy
set_location_assignment PIN_J2 -to ata_da[0] #cf_addr[0]
set_location_assignment PIN_J1 -to ata_da[1] #cf_addr[1]
set_location_assignment PIN_K1 -to ata_da[2] #cf_addr[2]
set_location_assignment PIN_J6 -to cf_gnd_da[3] #cf_addr[3]
set_location_assignment PIN_J5 -to cf_gnd_da[4] #cf_addr[4]
set_location_assignment PIN_H6 -to cf_gnd_da[5] #cf_addr[5]
set_location_assignment PIN_H5 -to cf_gnd_da[6] #cf_addr[6]
set_location_assignment PIN_G7 -to cf_gnd_da[7] #cf_addr[7]
set_location_assignment PIN_G6 -to cf_gnd_da[8] #cf_addr[8]
set_location_assignment PIN_M2  -to cf_gnd_da[9] #cf_addr[9]
set_location_assignment PIN_L3  -to cf_gnd_da[10] #cf_addr[10]
set_location_assignment PIN_AE8 -to cf_atasel
set_location_assignment PIN_K2  -to ata_cs0 #cf_cs_n[0]
set_location_assignment PIN_AE7 -to ata_cs1 #cf_cs_n[1]
set_location_assignment PIN_H3 -to ata_data[0]
set_location_assignment PIN_G3 -to ata_data[1]
set_location_assignment PIN_F3 -to ata_data[2]
set_location_assignment PIN_F1 -to ata_data[3]
set_location_assignment PIN_E3 -to ata_data[4]
set_location_assignment PIN_E1 -to ata_data[5]
set_location_assignment PIN_D2 -to ata_data[6]
set_location_assignment PIN_C1 -to ata_data[7]
set_location_assignment PIN_C2 -to ata_data[8]
set_location_assignment PIN_D3 -to ata_data[9]
set_location_assignment PIN_E2 -to ata_data[10]
set_location_assignment PIN_E4 -to ata_data[11]
set_location_assignment PIN_F2 -to ata_data[12]
set_location_assignment PIN_F4 -to ata_data[13]
set_location_assignment PIN_G4 -to ata_data[14]
set_location_assignment PIN_H4 -to ata_data[15]
set_location_assignment PIN_G1 -to ata_dior #cf_iord_n
set_location_assignment PIN_J4 -to ata_diow #cf_iowr_n
set_location_assignment PIN_AB12 -to cf_power
set_location_assignment PIN_J7 -to ata_dmack
set_location_assignment PIN_H7 -to cf_we

set_location_assignment PIN_J25 -to ssram_adsp_n
set_location_assignment PIN_J24 -to ssram_adv_n
set_location_assignment PIN_H16 -to bidir_port_to_and_from_the_reconfig_request_pio

#set_location_assignment PIN_J7 -to PROTO1_IO[40]

set_location_assignment PIN_T4 -to gpio[0]
set_location_assignment PIN_T5 -to gpio[11]
set_location_assignment PIN_U3 -to gpio[12]
set_location_assignment PIN_U4 -to gpio[13]
set_location_assignment PIN_T8 -to gpio[14]
set_location_assignment PIN_T9 -to gpio[15]

set_global_assignment -name STRATIXII_CONFIGURATION_SCHEME "ACTIVE SERIAL"
set_global_assignment -name GENERATE_TTF_FILE ON
set_global_assignment -name RESERVE_ALL_UNUSED_PINS "AS INPUT TRI-STATED"
set_global_assignment -name RESERVE_DATA0_AFTER_CONFIGURATION "AS INPUT TRI-STATED"
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
set_global_assignment -name STRATIXII_CONFIGURATION_DEVICE EPCS64
set_global_assignment -name RESERVE_ASDO_AFTER_CONFIGURATION "AS INPUT TRI-STATED"
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF

set_instance_assignment -name OUTPUT_ENABLE_GROUP 1 -to ddr_dm
set_instance_assignment -name OUTPUT_ENABLE_GROUP 1 -to ddr_dqs
set_instance_assignment -name OUTPUT_ENABLE_GROUP 1 -to ddr_dq
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_rasb
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_casb
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_web
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_cke
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[1]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[2]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[3]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[4]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[5]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[6]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[7]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[8]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[9]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[10]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[11]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ad[12]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ba[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_ba[1]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_csb
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dm[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dm[1]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[1]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[2]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[3]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[4]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[5]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[6]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[7]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[8]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[9]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[10]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[11]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[12]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[13]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[14]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dq[15]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dqs[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_dqs[1]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_clk #clk_to_sdram[0]
set_instance_assignment -name IO_STANDARD "SSTL-2 CLASS II" -to ddr_clkn #clk_to_sdram_n[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_rasb
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_casb
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_web
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_cke
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[1]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[2]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[3]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[4]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[5]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[6]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[7]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[8]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[9]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[10]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[11]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ad[12]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ba[0]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_ba[1]
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to ddr_csb
set_instance_assignment -name IO_STANDARD "2.5-V" -to clock_source
set_instance_assignment -name CUT ON -from ddr_dqs[0] -to *
set_instance_assignment -name CUT ON -from ddr_dqs[1] -to *
#set_location_assignment IOBANK_4 -to ddr_clk
#set_location_assignment IOBANK_4 -to ddr_clkn
set_global_assignment -name ASSIGNMENT_GROUP_MEMBER ddr_clk -section_id ddr_sdram_clk_out_pair
set_global_assignment -name ASSIGNMENT_GROUP_MEMBER ddr_clkn -section_id ddr_sdram_clk_out_pair
set_instance_assignment -name MAX_DATA_ARRIVAL_SKEW "100 ps" -from "ddrspa:\ddrsp0:ddrc0|ddr_phy:ddr_phy0|altera_ddr_phy:\alt:ddr_phy0|altpll:dll|_clk0" -to ddr_sdram_clk_out_pair
#set_instance_assignment -name MAX_DATA_ARRIVAL_SKEW "100 ps" -from "ddr_pll_stratixii:g_stratixpll_ddr_pll_inst|altpll:altpll_component|_clk0" -to ddr_sdram_clk_out_pair
#set_instance_assignment -name TPD_REQUIREMENT "1.6 ns" -from *captured_* -to *resynched_data*
set_instance_assignment -name ADV_NETLIST_OPT_ALLOWED "NEVER ALLOW" -to "full_2s60:inst|ddr_sdram:the_ddr_sdram|ddr_sdram_auk_ddr_sdram:ddr_sdram_auk_ddr_sdram_inst|ddr_sdram_auk_ddr_datapath:ddr_io|ddr_sdram_auk_ddr_dqs_group:\\g_datapath:0:g_ddr_io"
set_instance_assignment -name REMOVE_DUPLICATE_REGISTERS OFF -to "full_2s60:inst|ddr_sdram:the_ddr_sdram|ddr_sdram_auk_ddr_sdram:ddr_sdram_auk_ddr_sdram_inst|ddr_sdram_auk_ddr_datapath:ddr_io|ddr_sdram_auk_ddr_dqs_group:\\g_datapath:0:g_ddr_io"
set_location_assignment PIN_D9 -to ddr_dq[0]
set_location_assignment PIN_D8 -to ddr_dq[1]
set_location_assignment PIN_C8 -to ddr_dq[2]
set_location_assignment PIN_A9 -to ddr_dq[3]
set_location_assignment PIN_B11 -to ddr_dq[4]
set_location_assignment PIN_C11 -to ddr_dq[5]
set_location_assignment PIN_A10 -to ddr_dq[6]
set_location_assignment PIN_D10 -to ddr_dq[7]
set_location_assignment PIN_C9 -to ddr_dqs[0]
set_location_assignment PIN_C10 -to ddr_dm[0]
set_location_assignment PIN_A5 -to ddr_dq[8]
set_location_assignment PIN_B5 -to ddr_dq[9]
set_location_assignment PIN_D6 -to ddr_dq[10]
set_location_assignment PIN_A6 -to ddr_dq[11]
set_location_assignment PIN_A8 -to ddr_dq[12]
set_location_assignment PIN_A7 -to ddr_dq[13]
set_location_assignment PIN_C7 -to ddr_dq[14]
set_location_assignment PIN_D7 -to ddr_dq[15]
set_location_assignment PIN_C6 -to ddr_dqs[1]
set_location_assignment PIN_B7 -to ddr_dm[1]

set_global_assignment -name FMAX_REQUIREMENT "50.0 MHz"

#set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
#set_global_assignment -name PHYSICAL_SYNTHESIS_COMBO_LOGIC ON
#set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION ON
#set_global_assignment -name PHYSICAL_SYNTHESIS_ASYNCHRONOUS_SIGNAL_PIPELINING ON
#set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_RETIMING ON
#set_global_assignment -name PHYSICAL_SYNTHESIS_EFFORT EXTRA

set_global_assignment -name OPTIMIZE_HOLD_TIMING "ALL PATHS"
set_global_assignment -name OPTIMIZE_POWER_DURING_FITTING OFF
set_global_assignment -name ADV_NETLIST_OPT_SYNTH_WYSIWYG_REMAP ON
set_global_assignment -name ADV_NETLIST_OPT_SYNTH_GATE_RETIME ON
set_global_assignment -name STRATIXII_OPTIMIZATION_TECHNIQUE SPEED
set_global_assignment -name OPTIMIZE_POWER_DURING_SYNTHESIS OFF
set_global_assignment -name STATE_MACHINE_PROCESSING "ONE-HOT"

set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dm[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dm[1]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[1]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[2]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[3]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[4]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[5]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[6]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[7]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[8]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[9]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[10]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[11]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[12]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[13]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[14]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dq[15]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dqs[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 4 -to ddr_dqs[1]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_rasb
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_casb
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_web
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_cke
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[1]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[2]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[3]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[4]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[5]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[6]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[7]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[8]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[9]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[10]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[11]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ad[12]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ba[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_ba[1]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_csb
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_clk #clk_to_sdram[0]
set_instance_assignment -name OUTPUT_PIN_LOAD 2 -to ddr_clkn #clk_to_sdram_n[0]