#zc702 board

set_property PACKAGE_PIN P17 [get_ports {led[7]}]
set_property PACKAGE_PIN P18 [get_ports {led[6]}]
set_property PACKAGE_PIN W10 [get_ports {led[5]}]
set_property PACKAGE_PIN V7 [get_ports {led[4]}]
set_property PACKAGE_PIN W5 [get_ports {led[3]}]
set_property PACKAGE_PIN W17 [get_ports {led[2]}]
set_property PACKAGE_PIN D15 [get_ports {led[1]}]
set_property PACKAGE_PIN E15 [get_ports {led[0]}]

set_property IOSTANDARD LVCMOS18 [get_ports {led[7]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[6]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[5]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[4]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[3]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[2]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[1]}]
set_property IOSTANDARD LVCMOS18 [get_ports {led[0]}]

set_property PACKAGE_PIN G19 [get_ports {button[0]}]
set_property PACKAGE_PIN F19 [get_ports {button[1]}]
set_property PACKAGE_PIN J18 [get_ports {button[2]}] 
set_property PACKAGE_PIN K18 [get_ports {button[3]}] 

set_property PACKAGE_PIN N19 [get_ports {switch[0]}]
set_property PACKAGE_PIN N20 [get_ports {switch[1]}]
set_property PACKAGE_PIN N17 [get_ports {switch[2]}]
set_property PACKAGE_PIN N18 [get_ports {switch[3]}]
set_property PACKAGE_PIN M15 [get_ports {switch[4]}]
set_property PACKAGE_PIN M16 [get_ports {switch[5]}]
set_property PACKAGE_PIN P16 [get_ports {switch[6]}]
set_property PACKAGE_PIN R16 [get_ports {switch[7]}]

#create_clock -name clk100 -period 10.0 [get_ports gclk]
set_false_path -from  [get_clocks clk_fpga_0] -to [get_clocks clk_fpga_1]
set_false_path -from  [get_clocks clk_fpga_1] -to [get_clocks clk_fpga_0]


# Zedboard below
#NET led[0]              LOC = T22  | IOSTANDARD=LVCMOS33;  # "LD0"
#NET led[1]              LOC = T21  | IOSTANDARD=LVCMOS33;  # "LD1"
#NET led[2]              LOC = U22  | IOSTANDARD=LVCMOS33;  # "LD2"
#NET led[3]              LOC = U21  | IOSTANDARD=LVCMOS33;  # "LD3"
#NET led[4]              LOC = V22  | IOSTANDARD=LVCMOS33;  # "LD4"
#NET led[5]              LOC = W22  | IOSTANDARD=LVCMOS33;  # "LD5"
#NET led[6]              LOC = U19  | IOSTANDARD=LVCMOS33;  # "LD6"
#NET led[7]              LOC = U14  | IOSTANDARD=LVCMOS33;  # "LD7" 

#NET button[0]           LOC = R16  | IOSTANDARD=LVCMOS18;  # "BTND"
#NET button[1]           LOC = N15  | IOSTANDARD=LVCMOS18;  # "BTNL"
#NET button[2]           LOC = R18  | IOSTANDARD=LVCMOS18;  # "BTNR"
#NET button[3]           LOC = T18  | IOSTANDARD=LVCMOS18;  # "BTNU"

#NET switch[0]           LOC = F22  | IOSTANDARD=LVCMOS18;  # "SW0"
#NET switch[1]           LOC = G22  | IOSTANDARD=LVCMOS18;  # "SW1"
#NET switch[2]           LOC = H22  | IOSTANDARD=LVCMOS18;  # "SW2"
#NET switch[3]           LOC = F21  | IOSTANDARD=LVCMOS18;  # "SW3"
#NET switch[4]           LOC = H19  | IOSTANDARD=LVCMOS18;  # "SW4"
#NET switch[5]           LOC = H18  | IOSTANDARD=LVCMOS18;  # "SW5"
#NET switch[6]           LOC = H17  | IOSTANDARD=LVCMOS18;  # "SW6"
#NET switch[7]           LOC = M15  | IOSTANDARD=LVCMOS18;  # "SW7"
