##############################################################
#
# Xilinx Core Generator version 13.2
# Date: Wed Aug  8 14:55:22 2012
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
#  Generated from component: xilinx.com:ip:v6_pcie:1.7
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = VHDL
SET device = xc6vlx240t
SET devicefamily = virtex6
SET flowvendor = Other
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = ff1156
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -1
SET verilogsim = false
SET vhdlsim = true
# END Project Options
# BEGIN Select
SELECT Virtex-6_Integrated_Block_for_PCI_Express family Xilinx,_Inc. 1.7
# END Select
# BEGIN Parameters
CSET acceptable_l0s_latency=Maximum_of_64_ns
CSET acceptable_l1_latency=No_limit
CSET ack_nak_timeout_func=Absolute
CSET ack_nak_timeout_value=0000
CSET bar0_64bit=false
CSET bar0_enabled=true
CSET bar0_prefetchable=false
CSET bar0_scale=Megabytes
CSET bar0_size=2
CSET bar0_type=Memory
CSET bar1_64bit=false
CSET bar1_enabled=false
CSET bar1_prefetchable=false
CSET bar1_scale=Kilobytes
CSET bar1_size=2
CSET bar1_type=N/A
CSET bar2_64bit=false
CSET bar2_enabled=false
CSET bar2_prefetchable=false
CSET bar2_scale=Bytes
CSET bar2_size=128
CSET bar2_type=N/A
CSET bar3_64bit=false
CSET bar3_enabled=false
CSET bar3_prefetchable=false
CSET bar3_scale=Kilobytes
CSET bar3_size=2
CSET bar3_type=N/A
CSET bar4_64bit=false
CSET bar4_enabled=false
CSET bar4_prefetchable=false
CSET bar4_scale=Kilobytes
CSET bar4_size=2
CSET bar4_type=N/A
CSET bar5_enabled=false
CSET bar5_prefetchable=false
CSET bar5_scale=Kilobytes
CSET bar5_size=2
CSET bar5_type=N/A
CSET base_class_menu=Simple_communication_controllers
CSET buf_opt_bma=false
CSET cardbus_cis_pointer=00000000
CSET class_code_base=05
CSET class_code_interface=00
CSET class_code_sub=00
CSET component_name=v6_pcie_v1_7
CSET cost_table=1
CSET cpl_finite=false
CSET cpl_timeout_disable_sup=false
CSET cpl_timeout_range=Range_B
CSET d0_pme_support=true
CSET d0_power_consumed=0
CSET d0_power_consumed_factor=0
CSET d0_power_dissipated=0
CSET d0_power_dissipated_factor=0
CSET d1_pme_support=true
CSET d1_power_consumed=0
CSET d1_power_consumed_factor=0
CSET d1_power_dissipated=0
CSET d1_power_dissipated_factor=0
CSET d1_support=false
CSET d2_pme_support=true
CSET d2_power_consumed=0
CSET d2_power_consumed_factor=0
CSET d2_power_dissipated=0
CSET d2_power_dissipated_factor=0
CSET d2_support=false
CSET d3_power_consumed=0
CSET d3_power_consumed_factor=0
CSET d3_power_dissipated=0
CSET d3_power_dissipated_factor=0
CSET d3cold_pme_support=false
CSET d3hot_pme_support=true
CSET de_emph=0
CSET device_id=0007
CSET device_port_type=PCI_Express_Endpoint_device
CSET device_specific_initialization=false
CSET disable_tx_aspm_l0s=false
CSET dll_link_active_cap=false
CSET downstream_link_num=00
CSET dsn_enabled=true
CSET en_route_err_cor=false
CSET en_route_err_ftl=false
CSET en_route_err_nfl=false
CSET en_route_inta=false
CSET en_route_intb=false
CSET en_route_intc=false
CSET en_route_intd=false
CSET en_route_pm_pme=false
CSET en_route_pme_to=false
CSET en_route_pme_to_ack=false
CSET en_route_unlock=false
CSET enable_ack_nak_timer=false
CSET enable_lane_reversal=false
CSET enable_replay_timer=true
CSET enable_slot_clock_cfg=true
CSET expansion_rom_enabled=false
CSET expansion_rom_scale=Kilobytes
CSET expansion_rom_size=2
CSET ext_pci_cfg_space=false
CSET ext_pci_cfg_space_addr=3FF
CSET extended_tag_field=false
CSET force_no_scrambling=false
CSET hw_auton_spd_disable=false
CSET intx_generation=true
CSET io_base_limit_registers=Disabled
CSET legacy_interrupt=INTA
CSET link_speed=2.5_GT/s
CSET max_payload_size=128_bytes
CSET maximum_link_width=X8
CSET msi_64b=true
CSET msi_enabled=true
CSET msi_vec_mask=false
CSET msix_enabled=false
CSET msix_pba_bir=BAR_0
CSET msix_pba_offset=0
CSET msix_table_bir=BAR_0
CSET msix_table_offset=0
CSET msix_table_size=1
CSET multiple_message_capable=1_vector
CSET no_soft_reset=true
CSET pci_cfg_space=false
CSET pci_cfg_space_addr=3F
CSET pcie_blk_locn=X0Y0
CSET pcie_cap_slot_implemented=false
CSET pcie_debug_ports=false
CSET perf_level=Good
CSET phantom_functions=No_function_number_bits_used
CSET pipe_pipeline=None
CSET prefetchable_memory_base_limit_registers=Disabled
CSET rcb=64_byte
CSET ref_clk_freq=100_MHz
CSET replay_timeout_func=Add
CSET replay_timeout_value=0026
CSET revision_id=00
CSET root_cap_crs=false
CSET slot_cap_attn_butn=false
CSET slot_cap_attn_ind=false
CSET slot_cap_elec_interlock=false
CSET slot_cap_hotplug_cap=false
CSET slot_cap_hotplug_surprise=false
CSET slot_cap_mrl=false
CSET slot_cap_no_cmd_comp_sup=false
CSET slot_cap_physical_slot_num=0
CSET slot_cap_pwr_ctrl=false
CSET slot_cap_pwr_ind=false
CSET slot_cap_pwr_limit_scale=0
CSET slot_cap_pwr_limit_value=0
CSET sub_class_interface_menu=Generic_XT_compatible_serial_controller
CSET subsystem_id=0007
CSET subsystem_vendor_id=10EE
CSET trans_buf_pipeline=None
CSET trgt_link_speed=4'h1
CSET trim_tlp_digest=false
CSET upconfigure_capable=true
CSET user_clk_freq=250_default
CSET vc_cap_enabled=false
CSET vc_cap_reject_snoop=false
CSET vendor_id=10EE
CSET vsec_enabled=false
CSET xlnx_ref_board=ML_605
# END Parameters
GENERATE
# CRC: 1ab9c854
