## This file is a general .ucf for the Nexys4 rev B board
## To use it in a project:
## - uncomment the lines corresponding to used pins
## - rename the used signals according to the project

## Clock signal
NET "clk"   LOC = "E3"	| IOSTANDARD = "LVCMOS33";					#Bank = 35, Pin name = IO_L12P_T1_MRCC_35,					Sch name = CLK100MHZ
NET "clk" TNM_NET = sys_clk_pin;
TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 100 MHz HIGH 50%; 

NET "eth_clk" TNM_NET = eth_clk;
NET "eth_clk90" TNM_NET = eth_clk90;
TIMESPEC TS_eth_clk = PERIOD eth_clk 50 MHz HIGH 50%;

NET "clkm" TNM_NET = clkm;
TIMESPEC "TS_clkm_eth_clk90" = FROM "clkm" TO "eth_clk90" TIG;
TIMESPEC "TS_eth_clk90_clkm" = FROM "eth_clk90" TO "clkm" TIG;

## Switches
NET "sw<0>"			LOC = "U9"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L21P_T3_DQS_34,					Sch name = SW0
NET "sw<1>"			LOC = "U8"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_25_34,							Sch name = SW1
NET "sw<2>"			LOC = "R7"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L23P_T3_34,						Sch name = SW2
NET "sw<3>"			LOC = "R6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L19P_T3_34,						Sch name = SW3
NET "sw<4>"			LOC = "R5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L19N_T3_VREF_34,					Sch name = SW4
NET "sw<5>"			LOC = "V7"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L20P_T3_34,						Sch name = SW5
NET "sw<6>"			LOC = "V6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L20N_T3_34,						Sch name = SW6
NET "sw<7>"			LOC = "V5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L10P_T1_34,						Sch name = SW7
NET "sw<8>"			LOC = "U4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L8P_T1-34,						Sch name = SW8
NET "sw<9>"			LOC = "V2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L9N_T1_DQS_34,					Sch name = SW9
NET "sw<10>"			LOC = "U2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L9P_T1_DQS_34,					Sch name = SW10
NET "sw<11>"			LOC = "T3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L11N_T1_MRCC_34,					Sch name = SW11
NET "sw<12>"			LOC = "T1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L17N_T2_34,						Sch name = SW12
NET "sw<13>"			LOC = "R3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L11P_T1_SRCC_34,					Sch name = SW13
NET "sw<14>"			LOC = "P3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L14N_T2_SRCC_34,					Sch name = SW14
NET "sw<15>"			LOC = "P4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L14P_T2_SRCC_34,					Sch name = SW15
 
## LEDs
NET "led<0>"			LOC = "T8"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L24N_T3_34,						Sch name = LED0
NET "led<1>"			LOC = "V9"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L21N_T3_DQS_34,					Sch name = LED1
NET "led<2>"			LOC = "R8"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L24P_T3_34,						Sch name = LED2
NET "led<3>"			LOC = "T6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L23N_T3_34,						Sch name = LED3
NET "led<4>"			LOC = "T5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L12P_T1_MRCC_34,					Sch name = LED4
NET "led<5>"			LOC = "T4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L12N_T1_MRCC_34,					Sch	name = LED5
NET "led<6>"			LOC = "U7"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L22P_T3_34,						Sch name = LED6
NET "led<7>"			LOC = "U6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L22N_T3_34,						Sch name = LED7
NET "led<8>"			LOC = "V4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L10N_T1_34,						Sch name = LED8
NET "led<9>"			LOC = "U3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L8N_T1_34,						Sch name = LED9
NET "led<10>"			LOC = "V1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L7N_T1_34,						Sch name = LED10
NET "led<11>"			LOC = "R1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L17P_T2_34,						Sch name = LED11
NET "led<12>"			LOC = "P5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L13N_T2_MRCC_34,					Sch name = LED12
NET "led<13>"			LOC = "U1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L7P_T1_34,						Sch name = LED13
NET "led<14>"			LOC = "R2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L15N_T2_DQS_34,					Sch name = LED14
NET "led<15>"			LOC = "P2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L15P_T2_DQS_34,					Sch name = LED15

#NET "RGB1_Red"			LOC = "K5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L5P_T0_34,						Sch name = LED16_R
#NET "RGB1_Green"		LOC = "F13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L5P_T0_AD9P_15,					Sch name = LED16_G
#NET "RGB1_Blue"		LOC = "F6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L19N_T3_VREF_35,					Sch name = LED16_B
#NET "RGB2_Red"			LOC = "K6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_0_34,								Sch name = LED17_R
#NET "RGB2_Green"		LOC = "H6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_24P_T3_35,						Sch name =  LED17_G
#NET "RGB2_Blue"		LOC = "L16"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L3N_T0_DQS_EMCCLK_14,			Sch name = LED17_B

## 7 segment display
#NET "seg<0>"			LOC = "L3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L2N_T0_34,						Sch name = CA
#NET "seg<1>"			LOC = "N1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L3N_T0_DQS_34,					Sch name = CB
#NET "seg<2>"			LOC = "L5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L6N_T0_VREF_34,					Sch name = CC
#NET "seg<3>"			LOC = "L4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L5N_T0_34,						Sch name = CD
#NET "seg<4>"			LOC = "K3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L2P_T0_34,						Sch name = CE
#NET "seg<5>"			LOC = "M2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L4N_T0_34,						Sch name = CF
#NET "seg<6>"			LOC = "L6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L6P_T0_34,						Sch name = CG

#NET "dp"				LOC = "M4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L16P_T2_34,						Sch name = DP

#NET "an<0>"			LOC = "N6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L18N_T2_34,						Sch name = AN0
#NET "an<1>"			LOC = "M6"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L18P_T2_34,						Sch name = AN1
#NET "an<2>"			LOC = "M3"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L4P_T0_34,						Sch name = AN2
#NET "an<3>"			LOC = "N5"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L13_T2_MRCC_34,					Sch name = AN3
#NET "an<4>"			LOC = "N2"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L3P_T0_DQS_34,					Sch name = AN4
#NET "an<5>"			LOC = "N4"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L16N_T2_34,						Sch name = AN5
#NET "an<6>"			LOC = "L1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L1P_T0_34,						Sch name = AN6
#NET "an<7>"			LOC = "M1"	| IOSTANDARD = "LVCMOS33";		#Bank = 34, Pin name = IO_L1N_T034,							Sch name = AN7

## Buttons
NET "btnCpuResetn"		LOC = "C12"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L3P_T0_DQS_AD1P_15,				Sch name = CPU_RESET
NET "btn<0>"			LOC = "E16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L11N_T1_SRCC_15,					Sch name = BTNC
NET "btn<1>"			LOC = "F15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L14P_T2_SRCC_15,					Sch name = BTNU
NET "btn<2>"			LOC = "T16"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L15N_T2_DQS_DOUT_CSO_B_14,	Sch name = BTNL
NET "btn<3>"			LOC = "V10"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L21P_T3_DQS_14,					Sch name = BTND
NET "btn<4>"			LOC = "R10"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_25_14,							Sch name = BTNR
 
## Pmod Header JA
#NET "JA<0>"			LOC = "B13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L1N_T0_AD0N_15,					Sch name = JA1
#NET "JA<1>"			LOC = "F14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L5N_T0_AD9N_15,					Sch name = JA2
#NET "JA<2>"			LOC = "D17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L16N_T2_A27_15,					Sch name = JA3
#NET "JA<3>"			LOC = "E17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L16P_T2_A28_15,					Sch name = JA4
#NET "JA<4>"			LOC = "G13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_0_15,								Sch name = JA7
#NET "JA<5>"			LOC = "C17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L20N_T3_A19_15,					Sch name = JA8
#NET "JA<6>"			LOC = "D18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L21N_T3_A17_15,					Sch name = JA9
#NET "JA<7>"			LOC = "E18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L21P_T3_DQS_15,					Sch name = JA10

## Pmod Header JB
#NET "JB<0>"			LOC = "G14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L15N_T2_DQS_ADV_B_15,				Sch name = JB1
#NET "JB<1>"			LOC = "P15"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L13P_T2_MRCC_14,					Sch name = JB2
#NET "JB<2>"			LOC = "V11"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L21N_T3_DQS_A06_D22_14,			Sch name = JB3
#NET "JB<3>"			LOC = "V15"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L16P_T2_CSI_B_14,				Sch name = JB4
#NET "JB<4>"			LOC = "K16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_25_15,							Sch name = JB7
#NET "JB<5>"			LOC = "R16"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L15P_T2_DQS_RWR_B_14,			Sch name = JB8
#NET "JB<6>"			LOC = "T9"  | IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L24P_T3_A01_D17_14,				Sch name = JB9
#NET "JB<7>"			LOC = "U11"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L19N_T3_A09_D25_VREF_14,			Sch name = JB10 
 
## Pmod Header JC
#NET "JC<0>"			LOC = "K2"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L23P_T3_35,						Sch name = JC1
#NET "JC<1>"			LOC = "E7"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L6P_T0_35,						Sch name = JC2
#NET "JC<2>"			LOC = "J3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L22P_T3_35,						Sch name = JC3
#NET "JC<3>"			LOC = "J4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L21P_T3_DQS_35,					Sch name = JC4
#NET "JC<4>"			LOC = "K1"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L23N_T3_35,						Sch name = JC7
#NET "JC<5>"			LOC = "E6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L5P_T0_AD13P_35,					Sch name = JC8
#NET "JC<6>"			LOC = "J2"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L22N_T3_35,						Sch name = JC9
#NET "JC<7>"			LOC = "G6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L19P_T3_35,						Sch name = JC10
 
## Pmod Header JD
#NET "JD<0>"			LOC = "H4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L21N_T2_DQS_35,					Sch name = JD1
#NET "JD<1>"			LOC = "H1"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L17P_T2_35,						Sch name = JD2
#NET "JD<2>"			LOC = "G1"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L17N_T2_35,						Sch name = JD3
#NET "JD<3>"			LOC = "G3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L20N_T3_35,						Sch name = JD4
#NET "JD<4>"			LOC = "H2"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L15P_T2_DQS_35,					Sch name = JD7
#NET "JD<5>"			LOC = "G4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L20P_T3_35,						Sch name = JD8
#NET "JD<6>"			LOC = "G2"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L15N_T2_DQS_35,					Sch name = JD9
#NET "JD<7>"			LOC = "F3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L13N_T2_MRCC_35,					Sch name = JD10
 
## Pmod Header JXADC
#NET "JXADC<0>"			LOC = "A13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L9P_T1_DQS_AD3P_15,				Sch name = XADC1_P -> XA1_P
#NET "JXADC<1>"			LOC = "A15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L8P_T1_AD10P_15,					Sch name = XADC2_P -> XA2_P
#NET "JXADC<2>"			LOC = "B16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L7P_T1_AD2P_15,					Sch name = XADC3_P -> XA3_P
#NET "JXADC<3>"			LOC = "B18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L10P_T1_AD11P_15,					Sch name = XADC4_P -> XA4_P
#NET "JXADC<4>"			LOC = "A14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L9N_T1_DQS_AD3N_15,				Sch name = XADC1_N -> XA1_N
#NET "JXADC<5>"			LOC = "A16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L8N_T1_AD10N_15,					Sch name = XADC2_N -> XA2_N
#NET "JXADC<6>"			LOC = "B17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L7N_T1_AD2N_15,					Sch name = XADC3_N -> XA3_N 
#NET "JXADC<7>"			LOC = "A18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L10N_T1_AD11N_15,					Sch name = XADC4_N -> XA4_N

## VGA Connector
#NET "vgaRed<0>"		LOC = "A3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L8N_T1_AD14N_35,					Sch name = VGA_R0
#NET "vgaRed<1>"		LOC = "B4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L7N_T1_AD6N_35,					Sch name = VGA_R1
#NET "vgaRed<2>"		LOC = "C5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L1N_T0_AD4N_35,					Sch name = VGA_R2
#NET "vgaRed<3>"		LOC = "A4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L8P_T1_AD14P_35,					Sch name = VGA_R3
#NET "vgaBlue<0>"		LOC = "B7"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L2P_T0_AD12P_35,					Sch name = VGA_B0
#NET "vgaBlue<1>"		LOC = "C7"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L4N_T0_35,						Sch name = VGA_B1
#NET "vgaBlue<2>"		LOC = "D7"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L6N_T0_VREF_35,					Sch name = VGA_B2
#NET "vgaBlue<3>"		LOC = "D8"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L4P_T0_35,						Sch name = VGA_B3
#NET "vgaGreen<0>"		LOC = "C6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L1P_T0_AD4P_35,					Sch name = VGA_G0
#NET "vgaGreen<1>"		LOC = "A5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L3N_T0_DQS_AD5N_35,				Sch name = VGA_G1
#NET "vgaGreen<2>"		LOC = "B6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L2N_T0_AD12N_35,					Sch name = VGA_G2
#NET "vgaGreen<3>"		LOC = "A6"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L3P_T0_DQS_AD5P_35,				Sch name = VGA_G3
#NET "Hsync"			LOC = "B11"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L4P_T0_15,						Sch name = VGA_HS
#NET "Vsync"			LOC = "B12"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L3N_T0_DQS_AD1N_15,				Sch name = VGA_BVS

## Micro SD Connector
#NET "sdReset"			LOC = "E2"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L14P_T2_SRCC_35,					Sch name = SD_RESET
#NET "sdCD"				LOC = "A1"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L9N_T1_DQS_AD7N_35,				Sch name = SD_CD
#NET "sdSCK"			LOC = "B1"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L9P_T1_DQS_AD7P_35,				Sch name = SD_SCK
#NET "sdCmd"			LOC = "C1"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L16N_T2_35,						Sch name = SD_CMD
#NET "sdData<0>"		LOC = "C2"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L16P_T2_35,							Sch name = SD_DAT0
#NET "sdData<1>" 		LOC = "E1"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L18N_T2_35,						Sch name = SD_DAT1
#NET "sdData<2>"		LOC = "F1"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L18P_T2_35,						Sch name = SD_DAT2
#NET "sdData<3>"		LOC = "D2"  | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L14N_T2_SRCC_35,					Sch name = SD_DAT3

## Accelerometer
#NET "aclMISO"			LOC = "D13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L6N_T0_VREF_15,					Sch name = ACL_MISO
#NET "aclMOSI"			LOC = "B14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L2N_T0_AD8N_15,					Sch name = ACL_MOSI
#NET "aclSCK"			LOC = "D15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L12P_T1_MRCC_15,					Sch name = ACL_SCLK
#NET "aclSS"			LOC = "C15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L12N_T1_MRCC_15,					Sch name = ACL_CSN
#NET "aclInt1"			LOC = "C16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L20P_T3_A20_15,					Sch name = ACL_INT1
#NET "aclInt2"			LOC = "E15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L11P_T1_SRCC_15,					Sch name = ACL_INT2

## Temperature Sensor
#NET "tmpSCL"			LOC = "F16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L14N_T2_SRCC_15,					Sch name = TMP_SCL
#NET "tmpSDA"			LOC = "G16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L13N_T2_MRCC_15,					Sch name = TMP_SDA
#NET "tmpInt"			LOC = "D14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L1P_T0_AD0P_15,					Sch name = TMP_INT
#NET "tmpCT"			LOC = "C14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L1N_T0_AD0N_15,					Sch name = TMP_CT

## Omnidirectional Microphone
#NET "micClk"			LOC = "J5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_25_35,								Sch name = M_CLK
#NET "micData"			LOC = "H5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L24N_T3_35,						Sch name = M_DATA
#NET "micLRSel"			LOC = "F5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_0_35,								Sch name = M_LRSEL

## PWM Audio Amplifier
#NET "ampPWM"			LOC = "A11"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L4N_T0_15,						Sch name = AUD_PWM
#NET "ampSD"			LOC = "D12"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L6P_T0_15,						Sch name = AUD_SD

## USB-RS232 Interface
NET "RsRx"				LOC = "C4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L7P_T1_AD6P_35,					Sch name = UART_TXD_IN
NET "RsTx"				LOC = "D4"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L11N_T1_SRCC_35,					Sch name = UART_RXD_OUT
#NET "RsCts"			LOC = "D3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L12N_T1_MRCC_35,					Sch name = UART_CTS
#NET "RsRts"			LOC = "E5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L5N_T0_AD13N_35,					Sch name = UART_RTS

## USB HID (PS/2)
#NET "PS2Clk"			LOC = "F4"	| PULLUP | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L13P_T2_MRCC_35,					Sch name = PS2_CLK
#NET "PS2Data"			LOC = "B2"	| PULLUP | IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L10N_T1_AD15N_35,					Sch name = PS2_DATA

## SMSC Ethernet PHY
NET "PhyMdc"			LOC = "C9"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L11P_T1_SRCC_16,					Sch name = ETH_MDC
NET "PhyMdio"			LOC = "A9"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L14N_T2_SRCC_16,					Sch name = ETH_MDIO
NET "PhyRstn"			LOC = "B3"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L10P_T1_AD15P_35,					Sch name = ETH_RSTN
NET "PhyCrs"			LOC = "D9"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L6N_T0_VREF_16,					Sch name = ETH_CRSDV
NET "PhyRxEr"			LOC = "C10"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L13N_T2_MRCC_16,					Sch name = ETH_RXERR
NET "PhyRxd<0>"			LOC = "D10"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L19N_T3_VREF_16,					Sch name = ETH_RXD0
NET "PhyRxd<1>"			LOC = "C11"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L13P_T2_MRCC_16,					Sch name = ETH_RXD1
NET "PhyTxEn"			LOC = "B9"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L11N_T1_SRCC_16,					Sch name = ETH_TXEN
NET "PhyTxd<0>"			LOC = "A10"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L14P_T2_SRCC_16,					Sch name = ETH_TXD0
NET "PhyTxd<1>"			LOC = "A8"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L12N_T1_MRCC_16,					Sch name = ETH_TXD1
NET "PhyClk50Mhz"		LOC = "D5"	| IOSTANDARD = "LVCMOS33";		#Bank = 35, Pin name = IO_L11P_T1_SRCC_35,					Sch name = ETH_REFCLK
#NET "PhyIntn"			LOC = "B8"	| IOSTANDARD = "LVCMOS33";		#Bank = 16, Pin name = IO_L12P_T1_MRCC_16,					Sch name = ETH_INTN

## Quad SPI Flash
NET "QspiSCK"			LOC = "E9"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = CCLK_0,							Sch name = QSPI_SCK
NET "QspiDB<0>"			LOC = "K17"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L1P_T0_D00_MOSI_14,			Sch name = QSPI_DQ0
NET "QspiDB<1>"			LOC = "K18"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L1N_T0_D01_DIN_14,			Sch name = QSPI_DQ1
NET "QspiDB<2>"			LOC = "L14"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L20_T0_D02_14,				Sch name = QSPI_DQ2
NET "QspiDB<3>"			LOC = "M14"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L2P_T0_D03_14,				Sch name = QSPI_DQ3
NET "QspiCSn"			LOC = "L13"	| IOSTANDARD = "LVCMOS33";		#Bank = CONFIG, Pin name = IO_L15N_T2_DQS_DOUT_CSO_B_14,	Sch name = QSPI_CSN

## Cellular RAM
NET "RamCLK"			LOC = "T15"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L14N_T2_SRCC_14,					Sch name = CRAM_CLK
NET "RamADV"			LOC = "T13"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L23P_T3_A03_D19_14,				Sch name = CRAM_ADVN
NET "RamCE"				LOC = "L18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L4P_T0_D04_14,					Sch name = CRAM_CEN
NET "RamCRE"			LOC = "J14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L19P_T3_A22_15,					Sch name = CRAM_CRE
NET "RamOE"				LOC = "H14"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L15P_T2_DQS_15,					Sch name = CRAM_OEN
NET "RamWE"				LOC = "R11"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_0_14,								Sch name = CRAM_WEN
NET "RamLB"				LOC = "J15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L24N_T3_RS0_15,					Sch name = CRAM_LBN
NET "RamUB"				LOC = "J13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L17N_T2_A25_15,					Sch name = CRAM_UBN
#NET "RamWait"			LOC = "T14"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L14P_T2_SRCC_14,					Sch name = CRAM_WAIT

NET "data<0>"			LOC = "R12"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L5P_T0_DQ06_14,					Sch name = CRAM_DQ0
NET "data<1>"			LOC = "T11"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L19P_T3_A10_D26_14,				Sch name = CRAM_DQ1
NET "data<2>"			LOC = "U12"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L20P_T3_A08)D24_14,				Sch name = CRAM_DQ2
NET "data<3>"			LOC = "R13"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L5N_T0_D07_14,					Sch name = CRAM_DQ3
NET "data<4>"			LOC = "U18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L17N_T2_A13_D29_14,				Sch name = CRAM_DQ4
NET "data<5>"			LOC = "R17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L12N_T1_MRCC_14,					Sch name = CRAM_DQ5
NET "data<6>"			LOC = "T18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L7N_T1_D10_14,					Sch name = CRAM_DQ6
NET "data<7>"			LOC = "R18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L7P_T1_D09_14,					Sch name = CRAM_DQ7
NET "data<8>"			LOC = "F18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L22N_T3_A16_15,					Sch name = CRAM_DQ8
NET "data<9>"			LOC = "G18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L22P_T3_A17_15,					Sch name = CRAM_DQ9
NET "data<10>"			LOC = "G17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_IO_L18N_T2_A23_15,				Sch name = CRAM_DQ10
NET "data<11>"			LOC = "M18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L4N_T0_D05_14,					Sch name = CRAM_DQ11
NET "data<12>"			LOC = "M17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L10N_T1_D15_14,					Sch name = CRAM_DQ12
NET "data<13>"			LOC = "P18"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L9N_T1_DQS_D13_14,				Sch name = CRAM_DQ13
NET "data<14>"			LOC = "N17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L9P_T1_DQS_14,					Sch name = CRAM_DQ14
NET "data<15>"			LOC = "P17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L12P_T1_MRCC_14,					Sch name = CRAM_DQ15

NET "address<0>"		LOC = "J18"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L23N_T3_FWE_B_15,					Sch name = CRAM_A0
NET "address<1>"		LOC = "H17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L18P_T2_A24_15,					Sch name = CRAM_A1
NET "address<2>"		LOC = "H15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L19N_T3_A21_VREF_15,				Sch name = CRAM_A2
NET "address<3>"		LOC = "J17"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L23P_T3_FOE_B_15,					Sch name = CRAM_A3
NET "address<4>"		LOC = "H16"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L13P_T2_MRCC_15,					Sch name = CRAM_A4
NET "address<5>"		LOC = "K15"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L24P_T3_RS1_15,					Sch name = CRAM_A5
NET "address<6>"		LOC = "K13"	| IOSTANDARD = "LVCMOS33";		#Bank = 15, Pin name = IO_L17P_T2_A26_15,					Sch name = CRAM_A6
NET "address<7>"		LOC = "N15"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L11P_T1_SRCC_14,					Sch name = CRAM_A7
NET "address<8>"		LOC = "V16"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L16N_T2_SRCC-14,					Sch name = CRAM_A8
NET "address<9>"		LOC = "U14"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L22P_T3_A05_D21_14,				Sch name = CRAM_A9
NET "address<10>"		LOC = "V14"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L22N_T3_A04_D20_14,				Sch name = CRAM_A10
NET "address<11>"		LOC = "V12"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L20N_T3_A07_D23_14,				Sch name = CRAM_A11
NET "address<12>"		LOC = "P14"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L8N_T1_D12_14,					Sch name = CRAM_A12
NET "address<13>"		LOC = "U16"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L18P_T2_A12_D28_14,				Sch name = CRAM_A13
NET "address<14>"		LOC = "R15"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L13N_T2_MRCC_14,					Sch name = CRAM_A14
NET "address<15>"		LOC = "N14"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L8P_T1_D11_14,					Sch name = CRAM_A15
NET "address<16>"		LOC = "N16"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L11N_T1_SRCC_14,					Sch name = CRAM_A16
NET "address<17>"		LOC = "M13"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L6N_T0_D08_VREF_14,				Sch name = CRAM_A17
NET "address<18>"		LOC = "V17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L18N_T2_A11_D27_14,				Sch name = CRAM_A18
NET "address<19>"		LOC = "U17"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L17P_T2_A14_D30_14,				Sch name = CRAM_A19
NET "address<20>"		LOC = "T10"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L24N_T3_A00_D16_14,				Sch name = CRAM_A20
NET "address<21>"		LOC = "M16"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L10P_T1_D14_14,					Sch name = CRAM_A21
NET "address<22>"		LOC = "U13"	| IOSTANDARD = "LVCMOS33";		#Bank = 14, Pin name = IO_L23N_T3_A02_D18_14,				Sch name = CRAM_A22
