JTAG2 Enable
CONFIG_DSU_JTAG2
  Say Y to enable a second JTAG debug link (JTAG-to-AHB). Some template
  designs use both a macro based interface as well as a generic (VHDL).
  See the README.txt file for the template design in question.
