# DE2-115 FPGA Board Configuration

## Pin Assignments:

- CLOCK
- Sma
- LED
- KEY
- EX_IO
- SW
- SEG7
- LCD
- RS232
- PS2 for Keyboard and Mouse
- SDCARD
- VGA
- Audio
- I2C for EEPROM
- I2C for Audio Tv-Decoder
- Ethernet 0
- Ethernet 1
- TV Decoder
- USB 2.0 OTG (Cypress CY7C67200)
- IR Receiver
- SDRAM
- SRAM
- Flash
- GPIO

## Pin Assignment Table:

##

CLOCK
Name | Location | Direction | Standard
--- | --- | --- | ---
CLOCK_50 | Y2 | input | 3.3-V LVTTL
CLOCK2_50 | AG14 | input | 3.3-V LVTTL
CLOCK3_50 | AG15 | input | 3.3-V LVTTL

##

Sma
Name | Location | Direction | Standard
--- | --- | --- | ---
SMA_CLKIN | AH14 | input | 3.3-V LVTTL
SMA_CLKOUT | AE23 | output | 3.3-V LVTTL

##

LED
Name | Location | Direction | Standard
--- | --- | --- | ---
LEDR[0] | G19 | output | 2.5 V
LEDR[1] | F19 | output | 2.5 V
LEDR[2] | E19 | output | 2.5 V
LEDR[3] | F21 | output | 2.5 V
LEDR[4] | F18 | output | 2.5 V
LEDR[5] | E18 | output | 2.5 V
LEDR[6] | J19 | output | 2.5 V
LEDR[7] | H19 | output | 2.5 V
LEDR[8] | J17 | output | 2.5 V
LEDR[9] | G17 | output | 2.5 V
LEDR[10] | J15 | output | 2.5 V
LEDR[11] | H16 | output | 2.5 V
LEDR[12] | J16 | output | 2.5 V
LEDR[13] | H17 | output | 2.5 V
LEDR[14] | F15 | output | 2.5 V
LEDR[15] | G15 | output | 2.5 V
LEDR[16] | G16 | output | 2.5 V
LEDR[17] | H15 | output | 2.5 V
LEDG[0] | E21 | output | 2.5 V
LEDG[1] | E22 | output | 2.5 V
LEDG[2] | E25 | output | 2.5 V
LEDG[3] | E24 | output | 2.5 V
LEDG[4] | H21 | output | 2.5 V
LEDG[5] | G20 | output | 2.5 V
LEDG[6] | G22 | output | 2.5 V
LEDG[7] | G21 | output | 2.5 V
LEDG[8] | F17 | output | 2.5 V

##

KEY
Name | Location | Direction | Standard
--- | --- | --- | ---
KEY[0] | M23 | input | 3.3-V LVTTL
KEY[1] | M21 | input | 3.3-V LVTTL
KEY[2] | N21 | input | 3.3-V LVTTL
KEY[3] | R24 | input | 3.3-V LVTTL

##

EX_IO
Name | Location | Direction | Standard
--- | --- | --- | ---
EX_IO[0] | J10 | inout | 3.3-V LVTTL
EX_IO[1] | J14 | inout | 3.3-V LVTTL
EX_IO[2] | H13 | inout | 3.3-V LVTTL
EX_IO[3] | H14 | inout | 3.3-V LVTTL
EX_IO[4] | F14 | inout | 3.3-V LVTTL
EX_IO[5] | E10 | inout | 3.3-V LVTTL
EX_IO[6] | D9 | inout | 3.3-V LVTTL

##

SW
Name | Location | Direction | Standard
--- | --- | --- | ---
SW[0] | AB28 | input | 3.3-V LVTTL
SW[1] | AC28 | input | 3.3-V LVTTL
SW[2] | AC27 | input | 3.3-V LVTTL
SW[3] | AD27 | input | 3.3-V LVTTL
SW[4] | AB27 | input | 3.3-V LVTTL
SW[5] | AC26 | input | 3.3-V LVTTL
SW[6] | AD26 | input | 3.3-V LVTTL
SW[7] | AB26 | input | 3.3-V LVTTL
SW[8] | AC25 | input | 3.3-V LVTTL
SW[9] | AB25 | input | 3.3-V LVTTL
SW[10] | AC24 | input | 3.3-V LVTTL
SW[11] | AB24 | input | 3.3-V LVTTL
SW[12] | AB23 | input | 3.3-V LVTTL
SW[13] | AA24 | input | 3.3-V LVTTL
SW[14] | AA23 | input | 3.3-V LVTTL
SW[15] | AA22 | input | 3.3-V LVTTL
SW[16] | Y24 | input | 3.3-V LVTTL
SW[17] | Y23 | input | 3.3-V LVTTL

##

SEG7
Name | Location | Direction | Standard
--- | --- | --- | ---
HEX0[0] | G18 | output | 2.5 V
HEX0[1] | F22 | output | 2.5 V
HEX0[2] | E17 | output | 2.5 V
HEX0[3] | L26 | output | 3.3-V LVTTL
HEX0[4] | L25 | output | 3.3-V LVTTL
HEX0[5] | J22 | output | 3.3-V LVTTL
HEX0[6] | H22 | output | 3.3-V LVTTL
HEX1[0] | M24 | output | 3.3-V LVTTL
HEX1[1] | Y22 | output | 3.3-V LVTTL
HEX1[2] | W21 | output | 3.3-V LVTTL
HEX1[3] | W22 | output | 3.3-V LVTTL
HEX1[4] | W25 | output | 3.3-V LVTTL
HEX1[5] | U23 | output | 3.3-V LVTTL
HEX1[6] | U24 | output | 3.3-V LVTTL
HEX2[0] | AA25 | output | 3.3-V LVTTL
HEX2[1] | AA26 | output | 3.3-V LVTTL
HEX2[2] | Y25 | output | 3.3-V LVTTL
HEX2[3] | W26 | output | 3.3-V LVTTL
HEX2[4] | Y26 | output | 3.3-V LVTTL
HEX2[5] | W27 | output | 3.3-V LVTTL
HEX2[6] | W28 | output | 3.3-V LVTTL
HEX3[0] | V21 | output | 3.3-V LVTTL
HEX3[1] | U21 | output | 3.3-V LVTTL
HEX3[2] | AB20 | output | 3.3-V LVTTL
HEX3[3] | AA21 | output | 3.3-V LVTTL
HEX3[4] | AD24 | output | 3.3-V LVTTL
HEX3[5] | AF23 | output | 3.3-V LVTTL
HEX3[6] | Y19 | output | 3.3-V LVTTL
HEX4[0] | AB19 | output | 3.3-V LVTTL
HEX4[1] | AA19 | output | 3.3-V LVTTL
HEX4[2] | AG21 | output | 3.3-V LVTTL
HEX4[3] | AH21 | output | 3.3-V LVTTL
HEX4[4] | AE19 | output | 3.3-V LVTTL
HEX4[5] | AF19 | output | 3.3-V LVTTL
HEX4[6] | AE18 | output | 3.3-V LVTTL
HEX5[0] | AD18 | output | 3.3-V LVTTL
HEX5[1] | AC18 | output | 3.3-V LVTTL
HEX5[2] | AB18 | output | 3.3-V LVTTL
HEX5[3] | AH19 | output | 3.3-V LVTTL
HEX5[4] | AG19 | output | 3.3-V LVTTL
HEX5[5] | AF18 | output | 3.3-V LVTTL
HEX5[6] | AH18 | output | 3.3-V LVTTL
HEX6[0] | AA17 | output | 3.3-V LVTTL
HEX6[1] | AB16 | output | 3.3-V LVTTL
HEX6[2] | AA16 | output | 3.3-V LVTTL
HEX6[3] | AB17 | output | 3.3-V LVTTL
HEX6[4] | AB15 | output | 3.3-V LVTTL
HEX6[5] | AA15 | output | 3.3-V LVTTL
HEX6[6] | AC17 | output | 3.3-V LVTTL
HEX7[0] | AD17 | output | 3.3-V LVTTL
HEX7[1] | AE17 | output | 3.3-V LVTTL
HEX7[2] | AG17 | output | 3.3-V LVTTL
HEX7[3] | AH17 | output | 3.3-V LVTTL
HEX7[4] | AF17 | output | 3.3-V LVTTL
HEX7[5] | AG18 | output | 3.3-V LVTTL
HEX7[6] | AA14 | output | 3.3-V LVTTL

##

LCD
Name | Location | Direction | Standard
--- | --- | --- | ---
LCD_DATA[0] | L3 | inout | 3.3-V LVTTL
LCD_DATA[1] | L1 | inout | 3.3-V LVTTL
LCD_DATA[2] | L2 | inout | 3.3-V LVTTL
LCD_DATA[3] | K7 | inout | 3.3-V LVTTL
LCD_DATA[4] | K1 | inout | 3.3-V LVTTL
LCD_DATA[5] | K2 | inout | 3.3-V LVTTL
LCD_DATA[6] | M3 | inout | 3.3-V LVTTL
LCD_DATA[7] | M5 | inout | 3.3-V LVTTL
LCD_BLON | L6 | output | 3.3-V LVTTL
LCD_RW | M1 | output | 3.3-V LVTTL
LCD_EN | L4 | output | 3.3-V LVTTL
LCD_RS | M2 | output | 3.3-V LVTTL
LCD_ON | L5 | output | 3.3-V LVTTL

##

RS232
Name | Location | Direction | Standard
--- | --- | --- | ---
UART_TXD | G9 | output | 3.3-V LVTTL
UART_RXD | G12 | input | 3.3-V LVTTL
UART_RTS | G14 | output | 3.3-V LVTTL
UART_CTS | J13 | input | 3.3-V LVTTL

##

PS2 for Keyboard and Mouse
Name | Location | Direction | Standard
--- | --- | --- | ---
PS2_CLK | G6 | inout | 3.3-V LVTTL
PS2_DAT | H5 | inout | 3.3-V LVTTL
PS2_CLK2 | G5 | inout | 3.3-V LVTTL
PS2_DAT2 | F5 | inout | 3.3-V LVTTL

##

SDCARD
Name | Location | Direction | Standard
--- | --- | --- | ---
SD_CMD | AD14 | inout | 3.3-V LVTTL
SD_CLK | AE13 | output | 3.3-V LVTTL
SD_WP_N | AF14 | input | 3.3-V LVTTL
SD_DAT[0] | AE14 | inout | 3.3-V LVTTL
SD_DAT[1] | AF13 | inout | 3.3-V LVTTL
SD_DAT[2] | AB14 | inout | 3.3-V LVTTL
SD_DAT[3] | AC14 | inout | 3.3-V LVTTL

##

VGA
Name | Location | Direction | Standard
--- | --- | --- | ---
VGA_HS | G13 | output | 3.3-V LVTTL
VGA_VS | C13 | output | 3.3-V LVTTL
VGA_SYNC_N | C10 | output | 3.3-V LVTTL
VGA_CLK | A12 | output | 3.3-V LVTTL
VGA_BLANK_N | F11 | output | 3.3-V LVTTL
VGA_R[0] | E12 | output | 3.3-V LVTTL
VGA_R[1] | E11 | output | 3.3-V LVTTL
VGA_R[2] | D10 | output | 3.3-V LVTTL
VGA_R[3] | F12 | output | 3.3-V LVTTL
VGA_R[4] | G10 | output | 3.3-V LVTTL
VGA_R[5] | J12 | output | 3.3-V LVTTL
VGA_R[6] | H8 | output | 3.3-V LVTTL
VGA_R[7] | H10 | output | 3.3-V LVTTL
VGA_G[0] | G8 | output | 3.3-V LVTTL
VGA_G[1] | G11 | output | 3.3-V LVTTL
VGA_G[2] | F8 | output | 3.3-V LVTTL
VGA_G[3] | H12 | output | 3.3-V LVTTL
VGA_G[4] | C8 | output | 3.3-V LVTTL
VGA_G[5] | B8 | output | 3.3-V LVTTL
VGA_G[6] | F10 | output | 3.3-V LVTTL
VGA_G[7] | C9 | output | 3.3-V LVTTL
VGA_B[0] | B10 | output | 3.3-V LVTTL
VGA_B[1] | A10 | output | 3.3-V LVTTL
VGA_B[2] | C11 | output | 3.3-V LVTTL
VGA_B[3] | B11 | output | 3.3-V LVTTL
VGA_B[4] | A11 | output | 3.3-V LVTTL
VGA_B[5] | C12 | output | 3.3-V LVTTL
VGA_B[6] | D11 | output | 3.3-V LVTTL
VGA_B[7] | D12 | output | 3.3-V LVTTL

##

Audio
Name | Location | Direction | Standard
--- | --- | --- | ---
AUD_ADCLRCK | C2 | inout | 3.3-V LVTTL
AUD_ADCDAT | D2 | input | 3.3-V LVTTL
AUD_DACLRCK | E3 | inout | 3.3-V LVTTL
AUD_DACDAT | D1 | output | 3.3-V LVTTL
AUD_XCK | E1 | output | 3.3-V LVTTL
AUD_BCLK | F2 | inout | 3.3-V LVTTL

##

I2C for EEPROM
Name | Location | Direction | Standard
--- | --- | --- | ---
EEP_I2C_SCLK | D14 | output | 3.3-V LVTTL
EEP_I2C_SDAT | E14 | inout | 3.3-V LVTTL

##

I2C for Audio Tv-Decoder
Name | Location | Direction | Standard
--- | --- | --- | ---
I2C_SCLK | B7 | output | 3.3-V LVTTL
I2C_SDAT | A8 | inout | 3.3-V LVTTL

##

Ethernet 0
Name | Location | Direction | Standard
--- | --- | --- | ---
ENETCLK_25 | A14 | input | 3.3-V LVTTL
ENET0_TX_DATA[0] | C18 | output | 2.5 V
ENET0_RX_DATA[0] | C16 | input | 2.5 V
ENET0_TX_DATA[1] | D19 | output | 2.5 V
ENET0_RX_DATA[1] | D16 | input | 2.5 V
ENET0_TX_DATA[2] | A19 | output | 2.5 V
ENET0_RX_DATA[2] | D17 | input | 2.5 V
ENET0_TX_DATA[3] | B19 | output | 2.5 V
ENET0_RX_DATA[3] | C15 | input | 2.5 V
ENET0_GTX_CLK | A17 | output | 2.5 V
ENET0_TX_EN | A18 | output | 2.5 V
ENET0_TX_ER | B18 | output | 2.5 V
ENET0_INT_N | A21 | input | 2.5 V
ENET0_RST_N | C19 | output | 2.5 V
ENET0_RX_DV | C17 | input | 2.5 V
ENET0_RX_ER | D18 | input | 2.5 V
ENET0_RX_CRS | D15 | input | 2.5 V
ENET0_RX_COL | E15 | input | 2.5 V
ENET0_RX_CLK | A15 | input | 2.5 V
ENET0_TX_CLK | B17 | input | 2.5 V
ENET0_MDC | C20 | output | 2.5 V
ENET0_MDIO | B21 | inout | 2.5 V
ENET0_LINK100 | C14 | input | 3.3-V LVTTL

##

Ethernet 1
Name | Location | Direction | Standard
--- | --- | --- | ---
ENET1_TX_DATA[0] | C25 | output | 2.5 V
ENET1_RX_DATA[0] | B23 | input | 2.5 V
ENET1_TX_DATA[1] | A26 | output | 2.5 V
ENET1_RX_DATA[1] | C21 | input | 2.5 V
ENET1_TX_DATA[2] | B26 | output | 2.5 V
ENET1_RX_DATA[2] | A23 | input | 2.5 V
ENET1_TX_DATA[3] | C26 | output | 2.5 V
ENET1_RX_DATA[3] | D21 | input | 2.5 V
ENET1_GTX_CLK | C23 | output | 2.5 V
ENET1_TX_EN | B25 | output | 2.5 V
ENET1_TX_ER | A25 | output | 2.5 V
ENET1_INT_N | D24 | input | 2.5 V
ENET1_RST_N | D22 | output | 2.5 V
ENET1_RX_DV | A22 | input | 2.5 V
ENET1_RX_ER | C24 | input | 2.5 V
ENET1_RX_CRS | D20 | input | 2.5 V
ENET1_RX_COL | B22 | input | 2.5 V
ENET1_RX_CLK | B15 | input | 2.5 V
ENET1_TX_CLK | C22 | input | 2.5 V
ENET1_MDC | D23 | output | 2.5 V
ENET1_MDIO | D25 | inout | 2.5 V
ENET1_LINK100 | D13 | input | 3.3-V LVTTL

##

TV Decoder
Name | Location | Direction | Standard
--- | --- | --- | ---
TD_HS | E5 | input | 3.3-V LVTTL
TD_VS | E4 | input | 3.3-V LVTTL
TD_CLK27 | B14 | input | 3.3-V LVTTL
TD_RESET_N | G7 | output | 3.3-V LVTTL
TD_DATA[0] | E8 | input | 3.3-V LVTTL
TD_DATA[1] | A7 | input | 3.3-V LVTTL
TD_DATA[2] | D8 | input | 3.3-V LVTTL
TD_DATA[3] | C7 | input | 3.3-V LVTTL
TD_DATA[4] | D7 | input | 3.3-V LVTTL
TD_DATA[5] | D6 | input | 3.3-V LVTTL
TD_DATA[6] | E7 | input | 3.3-V LVTTL
TD_DATA[7] | F7 | input | 3.3-V LVTTL

##

USB 2.0 OTG (Cypress CY7C67200)
Name | Location | Direction | Standard
--- | --- | --- | ---
OTG_DATA[0] | J6 | inout | 3.3-V LVTTL
OTG_DATA[1] | K4 | inout | 3.3-V LVTTL
OTG_DATA[2] | J5 | inout | 3.3-V LVTTL
OTG_DATA[3] | K3 | inout | 3.3-V LVTTL
OTG_DATA[4] | J4 | inout | 3.3-V LVTTL
OTG_DATA[5] | J3 | inout | 3.3-V LVTTL
OTG_DATA[6] | J7 | inout | 3.3-V LVTTL
OTG_DATA[7] | H6 | inout | 3.3-V LVTTL
OTG_DATA[8] | H3 | inout | 3.3-V LVTTL
OTG_DATA[9] | H4 | inout | 3.3-V LVTTL
OTG_DATA[10] | G1 | inout | 3.3-V LVTTL
OTG_DATA[11] | G2 | inout | 3.3-V LVTTL
OTG_DATA[12] | G3 | inout | 3.3-V LVTTL
OTG_DATA[13] | F1 | inout | 3.3-V LVTTL
OTG_DATA[14] | F3 | inout | 3.3-V LVTTL
OTG_DATA[15] | G4 | inout | 3.3-V LVTTL
OTG_ADDR[0] | H7 | output | 3.3-V LVTTL
OTG_ADDR[1] | C3 | output | 3.3-V LVTTL
OTG_INT | D5 | input | 3.3-V LVTTL
OTG_RST_N | C5 | output | 3.3-V LVTTL
OTG_CS_N | A3 | output | 3.3-V LVTTL
OTG_RD_N | B3 | output | 3.3-V LVTTL
OTG_WE_N | A4 | output | 3.3-V LVTTL

##

IR Receiver
Name | Location | Direction | Standard
--- | --- | --- | ---
IRDA_RXD | Y15 | input | 3.3-V LVTTL

##

SDRAM
Name | Location | Direction | Standard
--- | --- | --- | ---
DRAM_BA[0] | U7 | output | 3.3-V LVTTL
DRAM_BA[1] | R4 | output | 3.3-V LVTTL
DRAM_DQM[0] | U2 | output | 3.3-V LVTTL
DRAM_DQM[1] | W4 | output | 3.3-V LVTTL
DRAM_DQM[2] | K8 | output | 3.3-V LVTTL
DRAM_DQM[3] | N8 | output | 3.3-V LVTTL
DRAM_RAS_N | U6 | output | 3.3-V LVTTL
DRAM_CAS_N | V7 | output | 3.3-V LVTTL
DRAM_CKE | AA6 | output | 3.3-V LVTTL
DRAM_CLK | AE5 | output | 3.3-V LVTTL
DRAM_WE_N | V6 | output | 3.3-V LVTTL
DRAM_CS_N | T4 | output | 3.3-V LVTTL
DRAM_DQ[0] | W3 | inout | 3.3-V LVTTL
DRAM_DQ[1] | W2 | inout | 3.3-V LVTTL
DRAM_DQ[2] | V4 | inout | 3.3-V LVTTL
DRAM_DQ[3] | W1 | inout | 3.3-V LVTTL
DRAM_DQ[4] | V3 | inout | 3.3-V LVTTL
DRAM_DQ[5] | V2 | inout | 3.3-V LVTTL
DRAM_DQ[6] | V1 | inout | 3.3-V LVTTL
DRAM_DQ[7] | U3 | inout | 3.3-V LVTTL
DRAM_DQ[8] | Y3 | inout | 3.3-V LVTTL
DRAM_DQ[9] | Y4 | inout | 3.3-V LVTTL
DRAM_DQ[10] | AB1 | inout | 3.3-V LVTTL
DRAM_DQ[11] | AA3 | inout | 3.3-V LVTTL
DRAM_DQ[12] | AB2 | inout | 3.3-V LVTTL
DRAM_DQ[13] | AC1 | inout | 3.3-V LVTTL
DRAM_DQ[14] | AB3 | inout | 3.3-V LVTTL
DRAM_DQ[15] | AC2 | inout | 3.3-V LVTTL
DRAM_DQ[16] | M8 | inout | 3.3-V LVTTL
DRAM_DQ[17] | L8 | inout | 3.3-V LVTTL
DRAM_DQ[18] | P2 | inout | 3.3-V LVTTL
DRAM_DQ[19] | N3 | inout | 3.3-V LVTTL
DRAM_DQ[20] | N4 | inout | 3.3-V LVTTL
DRAM_DQ[21] | M4 | inout | 3.3-V LVTTL
DRAM_DQ[22] | M7 | inout | 3.3-V LVTTL
DRAM_DQ[23] | L7 | inout | 3.3-V LVTTL
DRAM_DQ[24] | U5 | inout | 3.3-V LVTTL
DRAM_DQ[25] | R7 | inout | 3.3-V LVTTL
DRAM_DQ[26] | R1 | inout | 3.3-V LVTTL
DRAM_DQ[27] | R2 | inout | 3.3-V LVTTL
DRAM_DQ[28] | R3 | inout | 3.3-V LVTTL
DRAM_DQ[29] | T3 | inout | 3.3-V LVTTL
DRAM_DQ[30] | U4 | inout | 3.3-V LVTTL
DRAM_DQ[31] | U1 | inout | 3.3-V LVTTL
DRAM_ADDR[0] | R6 | output | 3.3-V LVTTL
DRAM_ADDR[1] | V8 | output | 3.3-V LVTTL
DRAM_ADDR[2] | U8 | output | 3.3-V LVTTL
DRAM_ADDR[3] | P1 | output | 3.3-V LVTTL
DRAM_ADDR[4] | V5 | output | 3.3-V LVTTL
DRAM_ADDR[5] | W8 | output | 3.3-V LVTTL
DRAM_ADDR[6] | W7 | output | 3.3-V LVTTL
DRAM_ADDR[7] | AA7 | output | 3.3-V LVTTL
DRAM_ADDR[8] | Y5 | output | 3.3-V LVTTL
DRAM_ADDR[9] | Y6 | output | 3.3-V LVTTL
DRAM_ADDR[10] | R5 | output | 3.3-V LVTTL
DRAM_ADDR[11] | AA5 | output | 3.3-V LVTTL
DRAM_ADDR[12] | Y7 | output | 3.3-V LVTTL

##

SRAM
Name | Location | Direction | Standard
--- | --- | --- | ---
SRAM_ADDR[0] | AB7 | output | 3.3-V LVTTL
SRAM_ADDR[1] | AD7 | output | 3.3-V LVTTL
SRAM_ADDR[2] | AE7 | output | 3.3-V LVTTL
SRAM_ADDR[3] | AC7 | output | 3.3-V LVTTL
SRAM_ADDR[4] | AB6 | output | 3.3-V LVTTL
SRAM_ADDR[5] | AE6 | output | 3.3-V LVTTL
SRAM_ADDR[6] | AB5 | output | 3.3-V LVTTL
SRAM_ADDR[7] | AC5 | output | 3.3-V LVTTL
SRAM_ADDR[8] | AF5 | output | 3.3-V LVTTL
SRAM_ADDR[9] | T7 | output | 3.3-V LVTTL
SRAM_ADDR[10] | AF2 | output | 3.3-V LVTTL
SRAM_ADDR[11] | AD3 | output | 3.3-V LVTTL
SRAM_ADDR[12] | AB4 | output | 3.3-V LVTTL
SRAM_ADDR[13] | AC3 | output | 3.3-V LVTTL
SRAM_ADDR[14] | AA4 | output | 3.3-V LVTTL
SRAM_ADDR[15] | AB11 | output | 3.3-V LVTTL
SRAM_ADDR[16] | AC11 | output | 3.3-V LVTTL
SRAM_ADDR[17] | AB9 | output | 3.3-V LVTTL
SRAM_ADDR[18] | AB8 | output | 3.3-V LVTTL
SRAM_ADDR[19] | T8 | output | 3.3-V LVTTL
SRAM_DQ[0] | AH3 | inout | 3.3-V LVTTL
SRAM_DQ[1] | AF4 | inout | 3.3-V LVTTL
SRAM_DQ[2] | AG4 | inout | 3.3-V LVTTL
SRAM_DQ[3] | AH4 | inout | 3.3-V LVTTL
SRAM_DQ[4] | AF6 | inout | 3.3-V LVTTL
SRAM_DQ[5] | AG6 | inout | 3.3-V LVTTL
SRAM_DQ[6] | AH6 | inout | 3.3-V LVTTL
SRAM_DQ[7] | AF7 | inout | 3.3-V LVTTL
SRAM_DQ[8] | AD1 | inout | 3.3-V LVTTL
SRAM_DQ[9] | AD2 | inout | 3.3-V LVTTL
SRAM_DQ[10] | AE2 | inout | 3.3-V LVTTL
SRAM_DQ[11] | AE1 | inout | 3.3-V LVTTL
SRAM_DQ[12] | AE3 | inout | 3.3-V LVTTL
SRAM_DQ[13] | AE4 | inout | 3.3-V LVTTL
SRAM_DQ[14] | AF3 | inout | 3.3-V LVTTL
SRAM_DQ[15] | AG3 | inout | 3.3-V LVTTL
SRAM_UB_N | AC4 | output | 3.3-V LVTTL
SRAM_LB_N | AD4 | output | 3.3-V LVTTL
SRAM_CE_N | AF8 | output | 3.3-V LVTTL
SRAM_OE_N | AD5 | output | 3.3-V LVTTL
SRAM_WE_N | AE8 | output | 3.3-V LVTTL

##

Flash
Name | Location | Direction | Standard
--- | --- | --- | ---
FL_ADDR[0] | AG12 | output | 3.3-V LVTTL
FL_ADDR[1] | AH7 | output | 3.3-V LVTTL
FL_ADDR[2] | Y13 | output | 3.3-V LVTTL
FL_ADDR[3] | Y14 | output | 3.3-V LVTTL
FL_ADDR[4] | Y12 | output | 3.3-V LVTTL
FL_ADDR[5] | AA13 | output | 3.3-V LVTTL
FL_ADDR[6] | AA12 | output | 3.3-V LVTTL
FL_ADDR[7] | AB13 | output | 3.3-V LVTTL
FL_ADDR[8] | AB12 | output | 3.3-V LVTTL
FL_ADDR[9] | AB10 | output | 3.3-V LVTTL
FL_ADDR[10] | AE9 | output | 3.3-V LVTTL
FL_ADDR[11] | AF9 | output | 3.3-V LVTTL
FL_ADDR[12] | AA10 | output | 3.3-V LVTTL
FL_ADDR[13] | AD8 | output | 3.3-V LVTTL
FL_ADDR[14] | AC8 | output | 3.3-V LVTTL
FL_ADDR[15] | Y10 | output | 3.3-V LVTTL
FL_ADDR[16] | AA8 | output | 3.3-V LVTTL
FL_ADDR[17] | AH12 | output | 3.3-V LVTTL
FL_ADDR[18] | AC12 | output | 3.3-V LVTTL
FL_ADDR[19] | AD12 | output | 3.3-V LVTTL
FL_ADDR[20] | AE10 | output | 3.3-V LVTTL
FL_ADDR[21] | AD10 | output | 3.3-V LVTTL
FL_ADDR[22] | AD11 | output | 3.3-V LVTTL
FL_DQ[0] | AH8 | inout | 3.3-V LVTTL
FL_DQ[1] | AF10 | inout | 3.3-V LVTTL
FL_DQ[2] | AG10 | inout | 3.3-V LVTTL
FL_DQ[3] | AH10 | inout | 3.3-V LVTTL
FL_DQ[4] | AF11 | inout | 3.3-V LVTTL
FL_DQ[5] | AG11 | inout | 3.3-V LVTTL
FL_DQ[6] | AH11 | inout | 3.3-V LVTTL
FL_DQ[7] | AF12 | inout | 3.3-V LVTTL
FL_CE_N | AG7 | output | 3.3-V LVTTL
FL_OE_N | AG8 | output | 3.3-V LVTTL
FL_RST_N | AE11 | output | 3.3-V LVTTL
FL_RY | Y1 | input | 3.3-V LVTTL
FL_WE_N | AC10 | output | 3.3-V LVTTL
FL_WP_N | AE12 | output | 3.3-V LVTTL

##

GPIO connect to GPIO Default
Name | Location | Direction | Standard | GPIO Pin Index
--- | --- | --- | --- | ---
GPIO[0] | AB22 | inout | 3.3-V LVTTL | 1
GPIO[1] | AC15 | inout | 3.3-V LVTTL | 2
GPIO[2] | AB21 | inout | 3.3-V LVTTL | 3
GPIO[3] | Y17 | inout | 3.3-V LVTTL | 4
GPIO[4] | AC21 | inout | 3.3-V LVTTL | 5
GPIO[5] | Y16 | inout | 3.3-V LVTTL | 6
GPIO[6] | AD21 | inout | 3.3-V LVTTL | 7
GPIO[7] | AE16 | inout | 3.3-V LVTTL | 8
GPIO[8] | AD15 | inout | 3.3-V LVTTL | 9
GPIO[9] | AE15 | inout | 3.3-V LVTTL | 10
GPIO[10] | AC19 | inout | 3.3-V LVTTL | 13
GPIO[11] | AF16 | inout | 3.3-V LVTTL | 14
GPIO[12] | AD19 | inout | 3.3-V LVTTL | 15
GPIO[13] | AF15 | inout | 3.3-V LVTTL | 16
GPIO[14] | AF24 | inout | 3.3-V LVTTL | 17
GPIO[15] | AE21 | inout | 3.3-V LVTTL | 18
GPIO[16] | AF25 | inout | 3.3-V LVTTL | 19
GPIO[17] | AC22 | inout | 3.3-V LVTTL | 20
GPIO[18] | AE22 | inout | 3.3-V LVTTL | 21
GPIO[19] | AF21 | inout | 3.3-V LVTTL | 22
GPIO[20] | AF22 | inout | 3.3-V LVTTL | 23
GPIO[21] | AD22 | inout | 3.3-V LVTTL | 24
GPIO[22] | AG25 | inout | 3.3-V LVTTL | 25
GPIO[23] | AD25 | inout | 3.3-V LVTTL | 26
GPIO[24] | AH25 | inout | 3.3-V LVTTL | 27
GPIO[25] | AE25 | inout | 3.3-V LVTTL | 28
GPIO[26] | AG22 | inout | 3.3-V LVTTL | 31
GPIO[27] | AE24 | inout | 3.3-V LVTTL | 32
GPIO[28] | AH22 | inout | 3.3-V LVTTL | 33
GPIO[29] | AF26 | inout | 3.3-V LVTTL | 34
GPIO[30] | AE20 | inout | 3.3-V LVTTL | 35
GPIO[31] | AG23 | inout | 3.3-V LVTTL | 36
GPIO[32] | AF20 | inout | 3.3-V LVTTL | 37
GPIO[33] | AH26 | inout | 3.3-V LVTTL | 38
GPIO[34] | AH23 | inout | 3.3-V LVTTL | 39
GPIO[35] | AG26 | inout | 3.3-V LVTTL | 40