diff --git a/vendor/riscv/riscv-config/riscv_config/schemas/schema_isa.yaml b/vendor/riscv/riscv-config/riscv_config/schemas/schema_isa.yaml
index a7536375f..27e88d16f 100644
--- a/vendor/riscv/riscv-config/riscv_config/schemas/schema_isa.yaml
+++ b/vendor/riscv/riscv-config/riscv_config/schemas/schema_isa.yaml
@@ -523,9 +523,9 @@ hart_schema:
       schema:
         description:
           type: string
-          default: The mstatus register keeps track of and controls the hart’s current
+          default: The mstatus register keeps track of and controls the hart's current
             operating state.
-        address: {type: integer, default: 768, allowed: [768]}
+        address: {type: integer, default: 0x300, allowed: [0x300]}
         priv_mode: {type: string, default: M, allowed: [M]}
         reset-val:
           type: integer
@@ -1506,7 +1506,7 @@ hart_schema:
           type: string
           default: The mstatush register keeps track of and controls the hart’s current
             operating state.
-        address: {type: integer, default: 768, allowed: [768]}
+        address: {type: integer, default: 0x310, allowed: [0x310]}
         priv_mode: {type: string, default: M, allowed: [M]}
         reset-val:
           type: integer
