/* Copyright (c) 2018, Marcelo Samsoniuk
 * All rights reserved.
 * 
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions are met:
 * 
 * * Redistributions of source code must retain the above copyright notice, this
 *   list of conditions and the following disclaimer.
 * 
 * * Redistributions in binary form must reproduce the above copyright notice,
 *   this list of conditions and the following disclaimer in the documentation
 *   and/or other materials provided with the distribution.
 * 
 * * Neither the name of the copyright holder nor the names of its
 *   contributors may be used to endorse or promote products derived from
 *   this software without specific prior written permission.
 * 
 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
 * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
 * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
 * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
 * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
 * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
 * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
 * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

MEMORY
{
    /* 
        darkshell 
    */

    MEM (rwx)  : ORIGIN = 0x00000000, LENGTH = MLEN
}

SECTIONS
{
    .text :
    {
        *boot*.o(.text)
        *boot*.o(.rodata)

        /* enable this in order to use the uart boot! */

        . = 512;

        _text = .;
        *(.text*)
        _etext = .;
    } > MEM
    .data :
    {
        _data = .;
        *(.rodata*)
        *(.data*)
        _global = . + 0x800;
        *(.sbss*)    
        *(.bss*)
        *(.sdata*)
        *(.*)
        . = ALIGN(4);
	    _edata = .;

    } > MEM

   PROVIDE ( _stack = ORIGIN(MEM) + LENGTH(MEM) );
}
