NET "VTRXC" LOC ="AA5";
NET "VRP_BANK6" LOC ="AP18";
NET "VRP_BANK5" LOC ="P20";
NET "VRP_BANK23" LOC ="K34";
NET "VRP_BANK21" LOC ="AP36";
NET "VRP_BANK19" LOC ="G37";
NET "VRP_BANK18" LOC ="AD7";
NET "VRP_BANK17" LOC ="AH39";
NET "VRP_BANK15" LOC ="U37";
NET "VRP_BANK13" LOC ="AL40";
NET "VRP_BANK12" LOC ="P6";
NET "VRN_BANK6" LOC ="AR18";
NET "VRN_BANK5" LOC ="N20";
NET "VRN_BANK23" LOC ="L34";
NET "VRN_BANK21" LOC ="AP37";
NET "VRN_BANK19" LOC ="H36";
NET "VRN_BANK18" LOC ="AD6";
NET "VRN_BANK17" LOC ="AG39";
NET "VRN_BANK15" LOC ="V38";
NET "VRN_BANK13" LOC ="AK40";
NET "VRN_BANK12" LOC ="P5";
NET "VREF_DDR2" LOC ="T41";
NET "VDDA_SATACLK" LOC ="AA8";
NET "VDDA_SATACLK" LOC ="U10";
NET "VCC3_PCI" LOC ="L8";
NET "VCC3V3" LOC ="AG30";
NET "VCC2V5" LOC ="E26";
NET "VCC1V8" LOC ="AA38";
NET "VCC1V0" LOC ="AA14";
NET "USER_SMA_CLK_P" LOC ="K30";
NET "USER_SMA_CLK_N" LOC ="L30";
NET "USER_CLKSYS" LOC ="L29";
NET "USER_CLK2" LOC ="K29";
NET "UART1_TXD" LOC ="T10";
NET "UART1_RXD" LOC ="V11";
NET "UART1_RTS_B" LOC ="K9";
NET "UART1_CTS_B" LOC ="J8";
NET "UART0_TXD" LOC ="H9";
NET "UART0_RXD" LOC ="T11";
NET "UART0_RTS_B" LOC ="J7";
NET "UART0_CTS_B" LOC ="H8";
NET "TRC_TS6" LOC ="AR17";
NET "TRC_TS5" LOC ="AP17";
NET "TRC_TS4" LOC ="AT27";
NET "TRC_TS3" LOC ="AU28";
NET "TRC_TS2" LOC ="AT16";
NET "TRC_TS1" LOC ="AT17";
NET "TRC_TS0" LOC ="AT29";
NET "TRC_ES4" LOC ="AR15";
NET "TRC_ES3" LOC ="AT26";
NET "TRC_ES2" LOC ="AT15";
NET "TRC_ES1" LOC ="AN20";
NET "TRC_ES0" LOC ="AN19";
NET "TRC_CLK_R" LOC ="AR27";
NET "TRC_BS2_BR2" LOC ="AN18";
NET "TRC_BS1_BR1" LOC ="AM18";
NET "TRC_BS0_BR0" LOC ="AN26";
NET "TEST_MON_VREFP" LOC ="AB22";
NET "TEST_MON_VP0_P" LOC ="AA22";
NET "TEST_MON_VN0_N" LOC ="AB21";
NET "TEST_MON_AVDD" LOC ="Y22";
NET "SYSACE_MPWE" LOC ="AR8";
NET "SYSACE_MPOE" LOC ="AK10";
NET "SYSACE_MPIRQ" LOC ="AK9";
NET "SYSACE_MPD9" LOC ="AV5";
NET "SYSACE_MPD8" LOC ="AV6";
NET "SYSACE_MPD7" LOC ="AH11";
NET "SYSACE_MPD6" LOC ="AH10";
NET "SYSACE_MPD5" LOC ="AU6";
NET "SYSACE_MPD4" LOC ="AT5";
NET "SYSACE_MPD3" LOC ="AH9";
NET "SYSACE_MPD2" LOC ="AG9";
NET "SYSACE_MPD15" LOC ="AK8";
NET "SYSACE_MPD14" LOC ="AP8";
NET "SYSACE_MPD13" LOC ="AT7";
NET "SYSACE_MPD12" LOC ="AJ8";
NET "SYSACE_MPD11" LOC ="AJ10";
NET "SYSACE_MPD10" LOC ="AJ11";
NET "SYSACE_MPD1" LOC ="AR5";
NET "SYSACE_MPD0" LOC ="AT6";
NET "SYSACE_MPCE" LOC ="AN8";
NET "SYSACE_MPBRDY" LOC ="AN4";
NET "SYSACE_MPA6" LOC ="AG11";
NET "SYSACE_MPA5" LOC ="AG12";
NET "SYSACE_MPA4" LOC ="AM8";
NET "SYSACE_MPA3" LOC ="AM7";
NET "SYSACE_MPA2" LOC ="AM6";
NET "SYSACE_MPA1" LOC ="AN6";
NET "SYSACE_MPA0" LOC ="AR7";
NET "SYSACE_FPGA_CLK" LOC ="L17";
NET "SYSACE_FLASH_CFGA1" LOC ="AK12";
NET "SYSACE_FLASH_CFGA0" LOC ="AK13";
NET "SPI_DATA_OUT" LOC ="AP7";
NET "SPI_DATA_IN" LOC ="AP5";
NET "SPI_DATA_CS_B" LOC ="AL10";
NET "SPI_CLK" LOC ="AL9";
NET "SGMIICLK_QO_P" LOC ="C4";
NET "SGMIICLK_QO_N" LOC ="C3";
NET "SBR_PWG_RSM_RSTJ" LOC ="M17";
NET "SBR_NMI_R" LOC ="AU29";
NET "SBR_INTR_R" LOC ="K28";
NET "SBR_IDE_RST_B" LOC ="AR19";
NET "SATACLK_QO_P" LOC ="F4";
NET "SATACLK_QO_N" LOC ="F3";
NET "PM_IO_9_N" LOC ="J25";
NET "PM_IO_95_N" LOC ="AV34";
NET "PM_IO_94_P" LOC ="AV33";
NET "PM_IO_93_N" LOC ="AU33";
NET "PM_IO_92_P" LOC ="AU32";
NET "PM_IO_91_N" LOC ="AR34";
NET "PM_IO_90_P" LOC ="AR35";
NET "PM_IO_8_P" LOC ="K25";
NET "PM_IO_89_N" LOC ="AT34";
NET "PM_IO_88_P" LOC ="AU34";
NET "PM_IO_87_N" LOC ="AT35";
NET "PM_IO_86_P" LOC ="AU36";
NET "PM_IO_85_N" LOC ="AV36";
NET "PM_IO_84_P" LOC ="AV35";
NET "PM_IO_83_N" LOC ="AJ31";
NET "PM_IO_82_P" LOC ="AH31";
NET "PM_IO_81_N" LOC ="AG32";
NET "PM_IO_80_P" LOC ="AH33";
NET "PM_IO_7_N" LOC ="F17";
NET "PM_IO_79_N" LOC ="AG33";
NET "PM_IO_78_P" LOC ="AF32";
NET "PM_IO_77_N" LOC ="AF31";
NET "PM_IO_76_P" LOC ="AG31";
NET "PM_IO_75_N" LOC ="AF12";
NET "PM_IO_74_P" LOC ="AF11";
NET "PM_IO_73_N" LOC ="AE10";
NET "PM_IO_72_P" LOC ="AE9";
NET "PM_IO_71_N" LOC ="AF10";
NET "PM_IO_70_P" LOC ="AF9";
NET "PM_IO_6_P" LOC ="F16";
NET "PM_IO_69_N" LOC ="AE8";
NET "PM_IO_68_P" LOC ="AD8";
NET "PM_IO_67_N" LOC ="AE7";
NET "PM_IO_66_P" LOC ="AF7";
NET "PM_IO_65_N" LOC ="AD5";
NET "PM_IO_64_P" LOC ="AE5";
NET "PM_IO_63_N" LOC ="AG7";
NET "PM_IO_62_P" LOC ="AG6";
NET "PM_IO_61_N" LOC ="AF6";
NET "PM_IO_60_P" LOC ="AF5";
NET "PM_IO_5_N" LOC ="L25";
NET "PM_IO_59_N" LOC ="AC6";
NET "PM_IO_58_P" LOC ="AC5";
NET "PM_IO_57_N" LOC ="AB6";
NET "PM_IO_56_P" LOC ="AB7";
NET "PM_IO_55_N" LOC ="AH4";
NET "PM_IO_54_P" LOC ="AG4";
NET "PM_IO_53_N" LOC ="AD11";
NET "PM_IO_52_P" LOC ="AD10";
NET "PM_IO_51_N" LOC ="AH5";
NET "PM_IO_50_P" LOC ="AH6";
NET "PM_IO_4_P" LOC ="K24";
NET "PM_IO_49_N" LOC ="AC9";
NET "PM_IO_48_P" LOC ="AC8";
NET "PM_IO_47_N_J" LOC ="AJ5";
NET "PM_IO_46_P_J" LOC ="AJ6";
NET "PM_IO_45_N" LOC ="AB8";
NET "PM_IO_44_P" LOC ="AB9";
NET "PM_IO_43_N" LOC ="AK5";
NET "PM_IO_42_P" LOC ="AL5";
NET "PM_IO_41_N" LOC ="AC10";
NET "PM_IO_40_P" LOC ="AB11";
NET "PM_IO_3_N" LOC ="E17";
NET "PM_IO_3V_9_N" LOC ="U6";
NET "PM_IO_3V_8_N" LOC ="J5";
NET "PM_IO_3V_7_N" LOC ="M6";
NET "PM_IO_3V_6_P" LOC ="H6";
NET "PM_IO_3V_5_P" LOC ="N5";
NET "PM_IO_3V_4_P" LOC ="AA7";
NET "PM_IO_3V_3_P" LOC ="K4";
NET "PM_IO_3V_2_N" LOC ="K5";
NET "PM_IO_3V_25_N" LOC ="V6";
NET "PM_IO_3V_24_P" LOC ="T7";
NET "PM_IO_3V_23_N" LOC ="W7";
NET "PM_IO_3V_22_P" LOC ="L6";
NET "PM_IO_3V_21_N" LOC ="H5";
NET "PM_IO_3V_20_P" LOC ="G6";
NET "PM_IO_3V_1_N" LOC ="L5";
NET "PM_IO_3V_19_N" LOC ="T6";
NET "PM_IO_3V_18_P" LOC ="V5";
NET "PM_IO_3V_17_N" LOC ="N6";
NET "PM_IO_3V_16_N" LOC ="V8";
NET "PM_IO_3V_15_N" LOC ="W6";
NET "PM_IO_3V_14_P" LOC ="J6";
NET "PM_IO_3V_13_P" LOC ="U7";
NET "PM_IO_3V_12_P" LOC ="W8";
NET "PM_IO_3V_11_P" LOC ="Y7";
NET "PM_IO_3V_10_N" LOC ="AA6";
NET "PM_IO_3V_0_P" LOC ="W5";
NET "PM_IO_39_N" LOC ="AK7";
NET "PM_IO_38_P" LOC ="AJ7";
NET "PM_IO_37_N_J" LOC ="H30";
NET "PM_IO_36_P_J" LOC ="H29";
NET "PM_IO_35_N" LOC ="L19";
NET "PM_IO_34_P" LOC ="L20";
NET "PM_IO_33_N" LOC ="F29";
NET "PM_IO_32_P" LOC ="G29";
NET "PM_IO_31_N" LOC ="N18";
NET "PM_IO_30_P" LOC ="M18";
NET "PM_IO_2_P" LOC ="E18";
NET "PM_IO_29_N" LOC ="H28";
NET "PM_IO_28_P" LOC ="G28";
NET "PM_IO_27_N" LOC ="N19";
NET "PM_IO_26_P" LOC ="M19";
NET "PM_IO_25_N" LOC ="F27";
NET "PM_IO_24_P" LOC ="G27";
NET "PM_IO_23_N" LOC ="L26";
NET "PM_IO_22_P" LOC ="K27";
NET "PM_IO_21_N" LOC ="K19";
NET "PM_IO_20_P" LOC ="K18";
NET "PM_IO_1_N" LOC ="M24";
NET "PM_IO_19_N" LOC ="H18";
NET "PM_IO_18_P" LOC ="J18";
NET "PM_IO_17_N" LOC ="J27";
NET "PM_IO_16_P" LOC ="J28";
NET "PM_IO_15_N" LOC ="G17";
NET "PM_IO_14_P" LOC ="G18";
NET "PM_IO_13_N" LOC ="J26";
NET "PM_IO_12_P" LOC ="H26";
NET "PM_IO_11_N" LOC ="H16";
NET "PM_IO_10_P" LOC ="G16";
NET "PM_IO_0_P" LOC ="L24";
NET "PM_CLK_TOP" LOC ="M27";
NET "PM_CLK_BOT" LOC ="L14";
NET "PLB_BUS_ERROR" LOC ="AK24";
NET "PHY1_RESET_SGMII" LOC ="AL25";
NET "PHY1_MDIO" LOC ="AT32";
NET "PHY1_MDC" LOC ="AU31";
NET "PHY1_INT_SGMII" LOC ="AV31";
NET "PHY0_TXER" LOC ="AT31";
NET "PHY0_TXD3" LOC ="AN31";
NET "PHY0_TXD2" LOC ="AR32";
NET "PHY0_TXD1" LOC ="AP32";
NET "PHY0_TXD0" LOC ="AR33";
NET "PHY0_TXCTL_TXEN" LOC ="AP31";
NET "PHY0_TXCLK" LOC ="M26";
NET "PHY0_RXER" LOC ="AP33";
NET "PHY0_RXD3" LOC ="AM33";
NET "PHY0_RXD2" LOC ="AK33";
NET "PHY0_RXD1" LOC ="AJ33";
NET "PHY0_RXD0" LOC ="AJ32";
NET "PHY0_RXCTL_RXDV" LOC ="AN33";
NET "PHY0_RXCLK" LOC ="J17";
NET "PHY0_RESET" LOC ="AK32";
NET "PHY0_MDIO" LOC ="AL31";
NET "PHY0_MDC" LOC ="AM32";
NET "PHY0_INT" LOC ="AL32";
NET "PHY0_GTXCLK" LOC ="AM31";
NET "PCI_P_TRDY_B" LOC ="V10";
NET "PCI_P_STOP_B" LOC ="G9";
NET "PCI_P_SERR_B" LOC ="G8";
NET "PCI_P_RST_B" LOC ="H11";
NET "PCI_P_REQ4_B" LOC ="R7";
NET "PCI_P_REQ3_B" LOC ="F6";
NET "PCI_P_REQ2_B" LOC ="D7";
NET "PCI_P_REQ1_B" LOC ="R8";
NET "PCI_P_REQ0_B" LOC ="E7";
NET "PCI_P_PERR_B" LOC ="G7";
NET "PCI_P_PAR" LOC ="E8";
NET "PCI_P_LOCK_B" LOC ="J12";
NET "PCI_P_IRDY_B" LOC ="P8";
NET "PCI_P_INTD_B" LOC ="F11";
NET "PCI_P_INTC_B" LOC ="F12";
NET "PCI_P_INTB_B" LOC ="G11";
NET "PCI_P_INTA_B" LOC ="G12";
NET "PCI_P_GNT4_B" LOC ="E5";
NET "PCI_P_GNT3_B" LOC ="R9";
NET "PCI_P_GNT2_B" LOC ="F5";
NET "PCI_P_GNT1_B" LOC ="F7";
NET "PCI_P_GNT0_B" LOC ="T9";
NET "PCI_P_FRAME_B" LOC ="P7";
NET "PCI_P_DEVSEL_B" LOC ="F9";
NET "PCI_P_CLK5_R" LOC ="V9";
NET "PCI_P_CLK5" LOC ="L16";
NET "PCI_P_CLK4_R" LOC ="U11";
NET "PCI_P_CLK3_R" LOC ="M9";
NET "PCI_P_CLK1_R" LOC ="U9";
NET "PCI_P_CLK0_R" LOC ="U8";
NET "PCI_P_CBE3_B" LOC ="F15";
NET "PCI_P_CBE2_B" LOC ="N9";
NET "PCI_P_CBE1_B" LOC ="N8";
NET "PCI_P_CBE0_B" LOC ="E9";
NET "PCI_P_AD9" LOC ="P12";
NET "PCI_P_AD8" LOC ="E12";
NET "PCI_P_AD7" LOC ="D12";
NET "PCI_P_AD6" LOC ="P11";
NET "PCI_P_AD5" LOC ="N10";
NET "PCI_P_AD4" LOC ="D13";
NET "PCI_P_AD31" LOC ="F10";
NET "PCI_P_AD30" LOC ="K14";
NET "PCI_P_AD3" LOC ="E14";
NET "PCI_P_AD29" LOC ="K13";
NET "PCI_P_AD28" LOC ="K12";
NET "PCI_P_AD27" LOC ="J11";
NET "PCI_P_AD26" LOC ="J13";
NET "PCI_P_AD25" LOC ="H13";
NET "PCI_P_AD24" LOC ="H10";
NET "PCI_P_AD23" LOC ="J10";
NET "PCI_P_AD22" LOC ="H14";
NET "PCI_P_AD21" LOC ="H15";
NET "PCI_P_AD20" LOC ="K10";
NET "PCI_P_AD2" LOC ="R10";
NET "PCI_P_AD19" LOC ="L10";
NET "PCI_P_AD18" LOC ="L12";
NET "PCI_P_AD17" LOC ="L11";
NET "PCI_P_AD16" LOC ="G13";
NET "PCI_P_AD15" LOC ="G14";
NET "PCI_P_AD14" LOC ="M11";
NET "PCI_P_AD13" LOC ="M12";
NET "PCI_P_AD12" LOC ="F14";
NET "PCI_P_AD11" LOC ="E13";
NET "PCI_P_AD10" LOC ="N11";
NET "PCI_P_AD1" LOC ="P10";
NET "PCI_P_AD0" LOC ="E15";
NET "PCI_FPGA_IDSEL" LOC ="E10";
NET "PCIE_SLOTB_WAKE_B_R" LOC ="J30";
NET "PCIE_SLOTB_PRSNT2_B_R" LOC ="K15";
NET "PCIE_SLOTB_PERST_B" LOC ="L15";
NET "PCIE_SLOTA_WAKE_B_R" LOC ="K17";
NET "PCIE_SLOTA_PRSNT2_B_R" LOC ="M28";
NET "PCIE_SLOTA_PERST_B" LOC ="L27";
NET "OPB_BUS_ERROR" LOC ="AL19";
NET "LVDS_CLKEXT_P_C" LOC ="V4";
NET "LVDS_CLKEXT_N_C" LOC ="V3";
NET "IIC_THERM_B" LOC ="AN24";
NET "IIC_SDA_DVI" LOC ="M7";
NET "IIC_SCL_DVI" LOC ="L9";
NET "IIC_RESET_B" LOC ="AK19";
NET "IIC_IRQ_B" LOC ="AK25";
NET "IIC_ALERT_B" LOC ="AK18";
NET "GTP_VREF" LOC ="AA4";
NET "GTP_134_VTTTX" LOC ="AY13";
NET "GTP_134_VTTTX" LOC ="AY18";
NET "GTP_134_VTTRX" LOC ="AY14";
NET "GTP_134_TX1_P_C" LOC ="BA18";
NET "GTP_134_TX1_N_C" LOC ="BA17";
NET "GTP_134_TX0_P_C" LOC ="BA13";
NET "GTP_134_TX0_N_C" LOC ="BA14";
NET "GTP_134_RX1_P" LOC ="BB17";
NET "GTP_134_RX1_N" LOC ="BB16";
NET "GTP_134_RX0_P" LOC ="BB14";
NET "GTP_134_RX0_N" LOC ="BB15";
NET "GTP_134_AVCC_PLL" LOC ="AY17";
NET "GTP_134_AVCC" LOC ="AW16";
NET "GTP_134_AVCC" LOC ="AY16";
NET "GTP_132_VTTTX" LOC ="C13";
NET "GTP_132_VTTTX" LOC ="C18";
NET "GTP_132_VTTRX" LOC ="C17";
NET "GTP_132_TX1_P_C" LOC ="B13";
NET "GTP_132_TX1_N_C" LOC ="B14";
NET "GTP_132_TX0_P_C" LOC ="B18";
NET "GTP_132_TX0_N_C" LOC ="B17";
NET "GTP_132_RX1_P" LOC ="A14";
NET "GTP_132_RX1_N" LOC ="A15";
NET "GTP_132_RX0_P" LOC ="A17";
NET "GTP_132_RX0_N" LOC ="A16";
NET "GTP_132_AVCC_PLL" LOC ="C14";
NET "GTP_132_AVCC" LOC ="C15";
NET "GTP_132_AVCC" LOC ="D15";
NET "GTP_130_VTTTX" LOC ="AY12";
NET "GTP_130_VTTTX" LOC ="AY7";
NET "GTP_130_VTTRX" LOC ="AY8";
NET "GTP_130_TX1_P_C" LOC ="BA12";
NET "GTP_130_TX1_N_C" LOC ="BA11";
NET "GTP_130_TX0_P_C" LOC ="BA7";
NET "GTP_130_TX0_N_C" LOC ="BA8";
NET "GTP_130_RX1_P" LOC ="BB11";
NET "GTP_130_RX1_N" LOC ="BB10";
NET "GTP_130_RX0_P" LOC ="BB8";
NET "GTP_130_RX0_N" LOC ="BB9";
NET "GTP_130_AVCC_PLL" LOC ="AY11";
NET "GTP_130_AVCC" LOC ="AW10";
NET "GTP_130_AVCC" LOC ="AY10";
NET "GTP_128_VTTTX" LOC ="C12";
NET "GTP_128_VTTTX" LOC ="C7";
NET "GTP_128_VTTRX" LOC ="C11";
NET "GTP_128_TX1_P_C" LOC ="B7";
NET "GTP_128_TX1_N_C" LOC ="B8";
NET "GTP_128_TX0_P_C" LOC ="B12";
NET "GTP_128_TX0_N_C" LOC ="B11";
NET "GTP_128_RX1_P" LOC ="A8";
NET "GTP_128_RX1_N" LOC ="A9";
NET "GTP_128_RX0_P" LOC ="A11";
NET "GTP_128_RX0_N" LOC ="A10";
NET "GTP_128_AVCC_PLL" LOC ="C8";
NET "GTP_128_AVCC" LOC ="C9";
NET "GTP_128_AVCC" LOC ="D9";
NET "GTP_126_VTTTX" LOC ="AY1";
NET "GTP_126_VTTTX" LOC ="AY6";
NET "GTP_126_VTTRX" LOC ="AY2";
NET "GTP_126_TX1_P_C" LOC ="BA6";
NET "GTP_126_TX1_N_C" LOC ="BA5";
NET "GTP_126_TX0_P_C" LOC ="BA1";
NET "GTP_126_TX0_N_C" LOC ="BA2";
NET "GTP_126_RX1_P" LOC ="BB5";
NET "GTP_126_RX1_N" LOC ="BB4";
NET "GTP_126_RX0_P" LOC ="BB2";
NET "GTP_126_RX0_N" LOC ="BB3";
NET "GTP_126_AVCC_PLL" LOC ="AY5";
NET "GTP_126_AVCC" LOC ="AW5";
NET "GTP_126_AVCC" LOC ="AY3";
NET "GTP_124_VTTTX" LOC ="C1";
NET "GTP_124_VTTTX" LOC ="C6";
NET "GTP_124_VTTRX" LOC ="C5";
NET "GTP_124_TX1_P" LOC ="B1";
NET "GTP_124_TX1_N" LOC ="B2";
NET "GTP_124_TX0_P" LOC ="B6";
NET "GTP_124_TX0_N" LOC ="B5";
NET "GTP_124_RX1_P" LOC ="A2";
NET "GTP_124_RX1_N" LOC ="A3";
NET "GTP_124_RX0_P" LOC ="A5";
NET "GTP_124_RX0_N" LOC ="A4";
NET "GTP_124_RTERM" LOC ="Y5";
NET "GTP_124_AVCC_PLL" LOC ="C2";
NET "GTP_124_AVCC" LOC ="D4";
NET "GTP_124_AVCC" LOC ="D5";
NET "GTP_122_VTTTX" LOC ="AP3";
NET "GTP_122_VTTTX" LOC ="AW3";
NET "GTP_122_VTTRX" LOC ="AR3";
NET "GTP_122_TX1_P_C" LOC ="AW2";
NET "GTP_122_TX1_N_C" LOC ="AV2";
NET "GTP_122_TX0_P_C" LOC ="AP2";
NET "GTP_122_TX0_N_C" LOC ="AR2";
NET "GTP_122_RX1_P" LOC ="AV1";
NET "GTP_122_RX1_N" LOC ="AU1";
NET "GTP_122_RX0_P" LOC ="AR1";
NET "GTP_122_RX0_N" LOC ="AT1";
NET "GTP_122_AVCC_PLL" LOC ="AV3";
NET "GTP_122_AVCC" LOC ="AU3";
NET "GTP_122_AVCC" LOC ="AU4";
NET "GTP_120_VTTTX" LOC ="D3";
NET "GTP_120_VTTTX" LOC ="J3";
NET "GTP_120_VTTRX" LOC ="E3";
NET "GTP_120_TX1_P" LOC ="J2";
NET "GTP_120_TX1_N" LOC ="H2";
NET "GTP_120_TX0_P" LOC ="D2";
NET "GTP_120_TX0_N" LOC ="E2";
NET "GTP_120_RX1_P" LOC ="H1";
NET "GTP_120_RX1_N" LOC ="G1";
NET "GTP_120_RX0_P" LOC ="E1";
NET "GTP_120_RX0_N" LOC ="F1";
NET "GTP_120_AVCC_PLL" LOC ="H3";
NET "GTP_120_AVCC" LOC ="G3";
NET "GTP_120_AVCC" LOC ="G4";
NET "GTP_118_VTTTX" LOC ="AH3";
NET "GTP_118_VTTTX" LOC ="AN3";
NET "GTP_118_VTTRX" LOC ="AJ3";
NET "GTP_118_TX1_P" LOC ="AN2";
NET "GTP_118_TX1_N" LOC ="AM2";
NET "GTP_118_TX0_P" LOC ="AH2";
NET "GTP_118_TX0_N" LOC ="AJ2";
NET "GTP_118_RX1_P" LOC ="AM1";
NET "GTP_118_RX1_N" LOC ="AL1";
NET "GTP_118_RX0_P" LOC ="AJ1";
NET "GTP_118_RX0_N" LOC ="AK1";
NET "GTP_118_AVCC_PLL" LOC ="AM3";
NET "GTP_118_AVCC" LOC ="AL3";
NET "GTP_118_AVCC" LOC ="AL4";
NET "GTP_116_VTTTX" LOC ="K3";
NET "GTP_116_VTTTX" LOC ="R3";
NET "GTP_116_VTTRX" LOC ="L3";
NET "GTP_116_TX1_P" LOC ="R2";
NET "GTP_116_TX1_N" LOC ="P2";
NET "GTP_116_TX0_P" LOC ="K2";
NET "GTP_116_TX0_N" LOC ="L2";
NET "GTP_116_RX1_P" LOC ="P1";
NET "GTP_116_RX1_N" LOC ="N1";
NET "GTP_116_RX0_P" LOC ="L1";
NET "GTP_116_RX0_N" LOC ="M1";
NET "GTP_116_AVCC_PLL" LOC ="P3";
NET "GTP_116_AVCC" LOC ="N3";
NET "GTP_116_AVCC" LOC ="N4";
NET "GTP_114_VTTTX" LOC ="AB3";
NET "GTP_114_VTTTX" LOC ="AG3";
NET "GTP_114_VTTRX" LOC ="AC3";
NET "GTP_114_TX1_P" LOC ="AG2";
NET "GTP_114_TX1_N" LOC ="AF2";
NET "GTP_114_TX0_P" LOC ="AB2";
NET "GTP_114_TX0_N" LOC ="AC2";
NET "GTP_114_RX1_P" LOC ="AF1";
NET "GTP_114_RX1_N" LOC ="AE1";
NET "GTP_114_RX0_P" LOC ="AC1";
NET "GTP_114_RX0_N" LOC ="AD1";
NET "GTP_114_GTPCLK_P" LOC ="AD4";
NET "GTP_114_GTPCLK_N" LOC ="AD3";
NET "GTP_114_AVCC_PLL" LOC ="AF3";
NET "GTP_114_AVCC" LOC ="AE3";
NET "GTP_114_AVCC" LOC ="AE4";
NET "GTP_112_VTTTX" LOC ="AA3";
NET "GTP_112_VTTTX" LOC ="T3";
NET "GTP_112_VTTRX" LOC ="U3";
NET "GTP_112_TX1_P" LOC ="AA2";
NET "GTP_112_TX1_N" LOC ="Y2";
NET "GTP_112_TX0_P" LOC ="T2";
NET "GTP_112_TX0_N" LOC ="U2";
NET "GTP_112_RX1_P" LOC ="Y1";
NET "GTP_112_RX1_N" LOC ="W1";
NET "GTP_112_RX0_P" LOC ="U1";
NET "GTP_112_RX0_N" LOC ="V1";
NET "GTP_112_RREF" LOC ="AB4";
NET "GTP_112_AVCC_PLL" LOC ="Y3";
NET "GTP_112_AVCC" LOC ="W3";
NET "GTP_112_AVCC" LOC ="W4";
NET "GTP132_PCIE_SLOTA_CLK_P" LOC ="D16";
NET "GTP132_PCIE_SLOTA_CLK_N" LOC ="C16";
NET "GTP128_PCIE_SLOTB_CLK_P" LOC ="D10";
NET "GTP128_PCIE_SLOTB_CLK_N" LOC ="C10";
NET "GTP126_PCIE_SLOTA_CLK_P" LOC ="AW4";
NET "GTP126_PCIE_SLOTA_CLK_N" LOC ="AY4";
NET "GTP122_PCIE_SLOTA_CLK_P" LOC ="AT4";
NET "GTP122_PCIE_SLOTA_CLK_N" LOC ="AT3";
NET "FPGA_VBATT" LOC ="P30";
NET "FPGA_TMS" LOC ="AH15";
NET "FPGA_TDO" LOC ="AJ15";
NET "FPGA_TDI" LOC ="AH16";
NET "FPGA_TCK" LOC ="AG29";
NET "FPGA_SDA" LOC ="K8";
NET "FPGA_SCL" LOC ="L7";
NET "FPGA_PROG_B" LOC ="R29";
NET "FPGA_MODE_2" LOC ="AJ28";
NET "FPGA_MODE_1" LOC ="AH30";
NET "FPGA_MODE_0" LOC ="AH29";
NET "FPGA_LED_USER2" LOC ="AL24";
NET "FPGA_LED_USER1" LOC ="AM19";
NET "FPGA_LCD_RW" LOC ="Y9";
NET "FPGA_LCD_RS" LOC ="Y8";
NET "FPGA_LCD_E" LOC ="W10";
NET "FPGA_LCD_DB7" LOC ="Y10";
NET "FPGA_LCD_DB6" LOC ="AA9";
NET "FPGA_LCD_DB5" LOC ="AA10";
NET "FPGA_LCD_DB4" LOC ="AA11";
NET "FPGA_LCD_DB3" LOC ="T4";
NET "FPGA_LCD_DB2" LOC ="T5";
NET "FPGA_LCD_DB1" LOC ="R5";
NET "FPGA_LCD_DB0" LOC ="R4";
NET "FPGA_INIT" LOC ="T14";
NET "FPGA_HSWAP" LOC ="P15";
NET "FPGA_DX_P" LOC ="AC22";
NET "FPGA_DX_N" LOC ="AC21";
NET "FPGA_DONE" LOC ="R14";
NET "FPGA_CPU_RESET_B" LOC ="J15";
NET "FPGA_CCLK" LOC ="AH14";
NET "FPGA_A22" LOC ="AK14";
NET "FLASH_WE_B" LOC ="AM28";
NET "FLASH_WAIT" LOC ="W11";
NET "FLASH_RESET_B" LOC ="K7";
NET "FLASH_OE_B" LOC ="AM13";
NET "FLASH_D9" LOC ="AL15";
NET "FLASH_D8" LOC ="AL16";
NET "FLASH_D7" LOC ="AN13";
NET "FLASH_D6" LOC ="AP13";
NET "FLASH_D5" LOC ="AK28";
NET "FLASH_D4" LOC ="AK29";
NET "FLASH_D3" LOC ="AN14";
NET "FLASH_D2" LOC ="AM14";
NET "FLASH_D15" LOC ="AN30";
NET "FLASH_D14" LOC ="AP30";
NET "FLASH_D13" LOC ="AK17";
NET "FLASH_D12" LOC ="AL17";
NET "FLASH_D11" LOC ="AN29";
NET "FLASH_D10" LOC ="AP28";
NET "FLASH_D1" LOC ="AK27";
NET "FLASH_D0" LOC ="AJ26";
NET "FLASH_CLK" LOC ="AN28";
NET "FLASH_CE_B" LOC ="AL14";
NET "FLASH_ADV_B" LOC ="AL29";
NET "FLASH_A9" LOC ="N15";
NET "FLASH_A8" LOC ="N14";
NET "FLASH_A7" LOC ="N28";
NET "FLASH_A6" LOC ="N29";
NET "FLASH_A5" LOC ="M14";
NET "FLASH_A4" LOC ="M13";
NET "FLASH_A3" LOC ="N30";
NET "FLASH_A21" LOC ="AL30";
NET "FLASH_A20" LOC ="AM29";
NET "FLASH_A2" LOC ="M29";
NET "FLASH_A19" LOC ="N25";
NET "FLASH_A18" LOC ="P25";
NET "FLASH_A17" LOC ="P18";
NET "FLASH_A16" LOC ="P17";
NET "FLASH_A15" LOC ="P26";
NET "FLASH_A14" LOC ="N26";
NET "FLASH_A13" LOC ="M16";
NET "FLASH_A12" LOC ="N16";
NET "FLASH_A11" LOC ="P27";
NET "FLASH_A10" LOC ="P28";
NET "FLASH_A1" LOC ="N13";
NET "FLASH_A0" LOC ="P13";
NET "DVI_XCLK_P" LOC ="AG8";
NET "DVI_XCLK_N" LOC ="AH8";
NET "DVI_V" LOC ="AM17";
NET "DVI_RESET_B" LOC ="AM9";
NET "DVI_H" LOC ="AP27";
NET "DVI_GPIO1" LOC ="AN9";
NET "DVI_DE" LOC ="M8";
NET "DVI_D9" LOC ="AK15";
NET "DVI_D8" LOC ="AM16";
NET "DVI_D7" LOC ="AM27";
NET "DVI_D6" LOC ="AM26";
NET "DVI_D5" LOC ="AN15";
NET "DVI_D4" LOC ="AN16";
NET "DVI_D3" LOC ="AL27";
NET "DVI_D2" LOC ="AL26";
NET "DVI_D11" LOC ="AK30";
NET "DVI_D10" LOC ="AJ30";
NET "DVI_D1" LOC ="AP16";
NET "DVI_D0" LOC ="AP15";
NET "DIMM1_DDR2_WE_B" LOC ="V40";
NET "DIMM1_DDR2_S1_B" LOC ="AE37";
NET "DIMM1_DDR2_S0_B" LOC ="AU42";
NET "DIMM1_DDR2_RAS_B" LOC ="V41";
NET "DIMM1_DDR2_PLL_CLKIN_P" LOC ="Y39";
NET "DIMM1_DDR2_PLL_CLKIN_N" LOC ="Y38";
NET "DIMM1_DDR2_ODT1" LOC ="AF37";
NET "DIMM1_DDR2_ODT0" LOC ="AV41";
NET "DIMM1_DDR2_DQS8_P" LOC ="AH34";
NET "DIMM1_DDR2_DQS8_N" LOC ="AG34";
NET "DIMM1_DDR2_DQS7_P" LOC ="AF35";
NET "DIMM1_DDR2_DQS7_N" LOC ="AF36";
NET "DIMM1_DDR2_DQS6_P" LOC ="AE35";
NET "DIMM1_DDR2_DQS6_N" LOC ="AF34";
NET "DIMM1_DDR2_DQS5_P" LOC ="AT39";
NET "DIMM1_DDR2_DQS5_N" LOC ="AR39";
NET "DIMM1_DDR2_DQS4_P" LOC ="AV40";
NET "DIMM1_DDR2_DQS4_N" LOC ="AU39";
NET "DIMM1_DDR2_DQS3_P" LOC ="AR40";
NET "DIMM1_DDR2_DQS3_N" LOC ="AT40";
NET "DIMM1_DDR2_DQS2_P" LOC ="AC40";
NET "DIMM1_DDR2_DQS2_N" LOC ="AC39";
NET "DIMM1_DDR2_DQS1_P" LOC ="AE40";
NET "DIMM1_DDR2_DQS1_N" LOC ="AD40";
NET "DIMM1_DDR2_DQS0_P" LOC ="AB39";
NET "DIMM1_DDR2_DQS0_N" LOC ="AC38";
NET "DIMM1_DDR2_DQM8" LOC ="AD33";
NET "DIMM1_DDR2_DQM7" LOC ="AV39";
NET "DIMM1_DDR2_DQM6" LOC ="AK35";
NET "DIMM1_DDR2_DQM5" LOC ="AN40";
NET "DIMM1_DDR2_DQM4" LOC ="AG37";
NET "DIMM1_DDR2_DQM3" LOC ="AC36";
NET "DIMM1_DDR2_DQM2" LOC ="AP41";
NET "DIMM1_DDR2_DQM1" LOC ="AH41";
NET "DIMM1_DDR2_DQM0" LOC ="AC41";
NET "DIMM1_DDR2_DQ9" LOC ="AF42";
NET "DIMM1_DDR2_DQ8" LOC ="AE42";
NET "DIMM1_DDR2_DQ7" LOC ="AF41";
NET "DIMM1_DDR2_DQ63" LOC ="AN34";
NET "DIMM1_DDR2_DQ62" LOC ="AU38";
NET "DIMM1_DDR2_DQ61" LOC ="AR37";
NET "DIMM1_DDR2_DQ60" LOC ="AN36";
NET "DIMM1_DDR2_DQ6" LOC ="AF40";
NET "DIMM1_DDR2_DQ59" LOC ="AU37";
NET "DIMM1_DDR2_DQ58" LOC ="AT36";
NET "DIMM1_DDR2_DQ57" LOC ="AT37";
NET "DIMM1_DDR2_DQ56" LOC ="AP35";
NET "DIMM1_DDR2_DQ55" LOC ="AK34";
NET "DIMM1_DDR2_DQ54" LOC ="AR38";
NET "DIMM1_DDR2_DQ53" LOC ="AL36";
NET "DIMM1_DDR2_DQ52" LOC ="AE32";
NET "DIMM1_DDR2_DQ51" LOC ="AL34";
NET "DIMM1_DDR2_DQ50" LOC ="AM34";
NET "DIMM1_DDR2_DQ5" LOC ="AB42";
NET "DIMM1_DDR2_DQ49" LOC ="AM36";
NET "DIMM1_DDR2_DQ48" LOC ="AL35";
NET "DIMM1_DDR2_DQ47" LOC ="AN39";
NET "DIMM1_DDR2_DQ46" LOC ="AN38";
NET "DIMM1_DDR2_DQ45" LOC ="AK38";
NET "DIMM1_DDR2_DQ44" LOC ="AL39";
NET "DIMM1_DDR2_DQ43" LOC ="AP38";
NET "DIMM1_DDR2_DQ42" LOC ="AM37";
NET "DIMM1_DDR2_DQ41" LOC ="AP40";
NET "DIMM1_DDR2_DQ40" LOC ="AM38";
NET "DIMM1_DDR2_DQ4" LOC ="AB41";
NET "DIMM1_DDR2_DQ39" LOC ="AJ37";
NET "DIMM1_DDR2_DQ38" LOC ="AK39";
NET "DIMM1_DDR2_DQ37" LOC ="AG38";
NET "DIMM1_DDR2_DQ36" LOC ="AF39";
NET "DIMM1_DDR2_DQ35" LOC ="AM39";
NET "DIMM1_DDR2_DQ34" LOC ="AL37";
NET "DIMM1_DDR2_DQ33" LOC ="AH38";
NET "DIMM1_DDR2_DQ32" LOC ="AJ38";
NET "DIMM1_DDR2_DQ31" LOC ="AD37";
NET "DIMM1_DDR2_DQ30" LOC ="AD35";
NET "DIMM1_DDR2_DQ3" LOC ="AD41";
NET "DIMM1_DDR2_DQ29" LOC ="AC35";
NET "DIMM1_DDR2_DQ28" LOC ="AB34";
NET "DIMM1_DDR2_DQ27" LOC ="AE38";
NET "DIMM1_DDR2_DQ26" LOC ="AD36";
NET "DIMM1_DDR2_DQ25" LOC ="AC34";
NET "DIMM1_DDR2_DQ24" LOC ="AB36";
NET "DIMM1_DDR2_DQ23" LOC ="AT41";
NET "DIMM1_DDR2_DQ22" LOC ="AT42";
NET "DIMM1_DDR2_DQ21" LOC ="AM41";
NET "DIMM1_DDR2_DQ20" LOC ="AN41";
NET "DIMM1_DDR2_DQ2" LOC ="AD42";
NET "DIMM1_DDR2_DQ19" LOC ="AR42";
NET "DIMM1_DDR2_DQ18" LOC ="AP42";
NET "DIMM1_DDR2_DQ17" LOC ="AL42";
NET "DIMM1_DDR2_DQ16" LOC ="AK42";
NET "DIMM1_DDR2_DQ15" LOC ="AL41";
NET "DIMM1_DDR2_DQ14" LOC ="AJ42";
NET "DIMM1_DDR2_DQ13" LOC ="AH40";
NET "DIMM1_DDR2_DQ12" LOC ="AG42";
NET "DIMM1_DDR2_DQ11" LOC ="AJ40";
NET "DIMM1_DDR2_DQ10" LOC ="AJ41";
NET "DIMM1_DDR2_DQ1" LOC ="AB37";
NET "DIMM1_DDR2_DQ0" LOC ="AB38";
NET "DIMM1_DDR2_CKE1" LOC ="AE39";
NET "DIMM1_DDR2_CKE0" LOC ="AU41";
NET "DIMM1_DDR2_CB7" LOC ="AE33";
NET "DIMM1_DDR2_CB6" LOC ="AE34";
NET "DIMM1_DDR2_CB5" LOC ="AC33";
NET "DIMM1_DDR2_CB4" LOC ="AB32";
NET "DIMM1_DDR2_CB3" LOC ="AH36";
NET "DIMM1_DDR2_CB2" LOC ="AG36";
NET "DIMM1_DDR2_CB1" LOC ="AD32";
NET "DIMM1_DDR2_CB0" LOC ="AB33";
NET "DIMM1_DDR2_CAS_B" LOC ="Y42";
NET "DIMM1_DDR2_BA2" LOC ="AH35";
NET "DIMM1_DDR2_BA1" LOC ="AJ36";
NET "DIMM1_DDR2_BA0" LOC ="AJ35";
NET "DIMM1_DDR2_A9" LOC ="F42";
NET "DIMM1_DDR2_A8" LOC ="G42";
NET "DIMM1_DDR2_A7" LOC ="J42";
NET "DIMM1_DDR2_A6" LOC ="H41";
NET "DIMM1_DDR2_A5" LOC ="M42";
NET "DIMM1_DDR2_A4" LOC ="L42";
NET "DIMM1_DDR2_A3" LOC ="K42";
NET "DIMM1_DDR2_A2" LOC ="M41";
NET "DIMM1_DDR2_A13" LOC ="W41";
NET "DIMM1_DDR2_A12" LOC ="F41";
NET "DIMM1_DDR2_A11" LOC ="G41";
NET "DIMM1_DDR2_A10" LOC ="W42";
NET "DIMM1_DDR2_A1" LOC ="J41";
NET "DIMM1_DDR2_A0" LOC ="R40";
NET "DIMM0_DDR2_WE_B" LOC ="Y40";
NET "DIMM0_DDR2_S1_B" LOC ="M37";
NET "DIMM0_DDR2_S0_B" LOC ="U32";
NET "DIMM0_DDR2_RAS_B" LOC ="W40";
NET "DIMM0_DDR2_PLL_CLKIN_P" LOC ="AA40";
NET "DIMM0_DDR2_PLL_CLKIN_N" LOC ="AA39";
NET "DIMM0_DDR2_ODT1" LOC ="K35";
NET "DIMM0_DDR2_ODT0" LOC ="U31";
NET "DIMM0_DDR2_DQS8_P" LOC ="H40";
NET "DIMM0_DDR2_DQS8_N" LOC ="J40";
NET "DIMM0_DDR2_DQS7_P" LOC ="K38";
NET "DIMM0_DDR2_DQS7_N" LOC ="J38";
NET "DIMM0_DDR2_DQS6_P" LOC ="M38";
NET "DIMM0_DDR2_DQS6_N" LOC ="L39";
NET "DIMM0_DDR2_DQS5_P" LOC ="U36";
NET "DIMM0_DDR2_DQS5_N" LOC ="V36";
NET "DIMM0_DDR2_DQS4_P" LOC ="R35";
NET "DIMM0_DDR2_DQS4_N" LOC ="T36";
NET "DIMM0_DDR2_DQS3_P" LOC ="T34";
NET "DIMM0_DDR2_DQS3_N" LOC ="U33";
NET "DIMM0_DDR2_DQS2_P" LOC ="E32";
NET "DIMM0_DDR2_DQS2_N" LOC ="E33";
NET "DIMM0_DDR2_DQS1_P" LOC ="F31";
NET "DIMM0_DDR2_DQS1_N" LOC ="F32";
NET "DIMM0_DDR2_DQS0_P" LOC ="E34";
NET "DIMM0_DDR2_DQS0_N" LOC ="F34";
NET "DIMM0_DDR2_DQM8" LOC ="G39";
NET "DIMM0_DDR2_DQM7" LOC ="W36";
NET "DIMM0_DDR2_DQM6" LOC ="T39";
NET "DIMM0_DDR2_DQM5" LOC ="V35";
NET "DIMM0_DDR2_DQM4" LOC ="M36";
NET "DIMM0_DDR2_DQM3" LOC ="F36";
NET "DIMM0_DDR2_DQM2" LOC ="P33";
NET "DIMM0_DDR2_DQM1" LOC ="L32";
NET "DIMM0_DDR2_DQM0" LOC ="F35";
NET "DIMM0_DDR2_DQ9" LOC ="L31";
NET "DIMM0_DDR2_DQ8" LOC ="J33";
NET "DIMM0_DDR2_DQ7" LOC ="H34";
NET "DIMM0_DDR2_DQ63" LOC ="W35";
NET "DIMM0_DDR2_DQ62" LOC ="W37";
NET "DIMM0_DDR2_DQ61" LOC ="T37";
NET "DIMM0_DDR2_DQ60" LOC ="P37";
NET "DIMM0_DDR2_DQ6" LOC ="H31";
NET "DIMM0_DDR2_DQ59" LOC ="Y34";
NET "DIMM0_DDR2_DQ58" LOC ="AA34";
NET "DIMM0_DDR2_DQ57" LOC ="AA36";
NET "DIMM0_DDR2_DQ56" LOC ="AA35";
NET "DIMM0_DDR2_DQ55" LOC ="V39";
NET "DIMM0_DDR2_DQ54" LOC ="R37";
NET "DIMM0_DDR2_DQ53" LOC ="R39";
NET "DIMM0_DDR2_DQ52" LOC ="N38";
NET "DIMM0_DDR2_DQ51" LOC ="W38";
NET "DIMM0_DDR2_DQ50" LOC ="Y35";
NET "DIMM0_DDR2_DQ5" LOC ="G33";
NET "DIMM0_DDR2_DQ49" LOC ="P38";
NET "DIMM0_DDR2_DQ48" LOC ="U38";
NET "DIMM0_DDR2_DQ47" LOC ="W33";
NET "DIMM0_DDR2_DQ46" LOC ="Y33";
NET "DIMM0_DDR2_DQ45" LOC ="T35";
NET "DIMM0_DDR2_DQ44" LOC ="R34";
NET "DIMM0_DDR2_DQ43" LOC ="AA32";
NET "DIMM0_DDR2_DQ42" LOC ="Y32";
NET "DIMM0_DDR2_DQ41" LOC ="W32";
NET "DIMM0_DDR2_DQ40" LOC ="V33";
NET "DIMM0_DDR2_DQ4" LOC ="G32";
NET "DIMM0_DDR2_DQ39" LOC ="P35";
NET "DIMM0_DDR2_DQ38" LOC ="N36";
NET "DIMM0_DDR2_DQ37" LOC ="L36";
NET "DIMM0_DDR2_DQ36" LOC ="J35";
NET "DIMM0_DDR2_DQ35" LOC ="U34";
NET "DIMM0_DDR2_DQ34" LOC ="V34";
NET "DIMM0_DDR2_DQ33" LOC ="P36";
NET "DIMM0_DDR2_DQ32" LOC ="N35";
NET "DIMM0_DDR2_DQ31" LOC ="J37";
NET "DIMM0_DDR2_DQ30" LOC ="H35";
NET "DIMM0_DDR2_DQ3" LOC ="H33";
NET "DIMM0_DDR2_DQ29" LOC ="E38";
NET "DIMM0_DDR2_DQ28" LOC ="D37";
NET "DIMM0_DDR2_DQ27" LOC ="K37";
NET "DIMM0_DDR2_DQ26" LOC ="J36";
NET "DIMM0_DDR2_DQ25" LOC ="G36";
NET "DIMM0_DDR2_DQ24" LOC ="F37";
NET "DIMM0_DDR2_DQ23" LOC ="T31";
NET "DIMM0_DDR2_DQ22" LOC ="R32";
NET "DIMM0_DDR2_DQ21" LOC ="P31";
NET "DIMM0_DDR2_DQ20" LOC ="N34";
NET "DIMM0_DDR2_DQ2" LOC ="J31";
NET "DIMM0_DDR2_DQ19" LOC ="T32";
NET "DIMM0_DDR2_DQ18" LOC ="R33";
NET "DIMM0_DDR2_DQ17" LOC ="P32";
NET "DIMM0_DDR2_DQ16" LOC ="N33";
NET "DIMM0_DDR2_DQ15" LOC ="N31";
NET "DIMM0_DDR2_DQ14" LOC ="M32";
NET "DIMM0_DDR2_DQ13" LOC ="K33";
NET "DIMM0_DDR2_DQ12" LOC ="K32";
NET "DIMM0_DDR2_DQ11" LOC ="M34";
NET "DIMM0_DDR2_DQ10" LOC ="M33";
NET "DIMM0_DDR2_DQ1" LOC ="G31";
NET "DIMM0_DDR2_DQ0" LOC ="E35";
NET "DIMM0_DDR2_CKE1" LOC ="L37";
NET "DIMM0_DDR2_CKE0" LOC ="M31";
NET "DIMM0_DDR2_CB7" LOC ="H39";
NET "DIMM0_DDR2_CB6" LOC ="G38";
NET "DIMM0_DDR2_CB5" LOC ="E39";
NET "DIMM0_DDR2_CB4" LOC ="E40";
NET "DIMM0_DDR2_CB3" LOC ="H38";
NET "DIMM0_DDR2_CB2" LOC ="K40";
NET "DIMM0_DDR2_CB1" LOC ="F39";
NET "DIMM0_DDR2_CB0" LOC ="F40";
NET "DIMM0_DDR2_CAS_B" LOC ="AA37";
NET "DIMM0_DDR2_BA2" LOC ="K39";
NET "DIMM0_DDR2_BA1" LOC ="M39";
NET "DIMM0_DDR2_BA0" LOC ="N39";
NET "DIMM0_DDR2_A9" LOC ="L40";
NET "DIMM0_DDR2_A8" LOC ="P42";
NET "DIMM0_DDR2_A7" LOC ="R42";
NET "DIMM0_DDR2_A6" LOC ="P41";
NET "DIMM0_DDR2_A5" LOC ="T40";
NET "DIMM0_DDR2_A4" LOC ="U42";
NET "DIMM0_DDR2_A3" LOC ="T42";
NET "DIMM0_DDR2_A2" LOC ="U41";
NET "DIMM0_DDR2_A13" LOC ="Y37";
NET "DIMM0_DDR2_A12" LOC ="N41";
NET "DIMM0_DDR2_A11" LOC ="N40";
NET "DIMM0_DDR2_A10" LOC ="AA41";
NET "DIMM0_DDR2_A1" LOC ="P40";
NET "DIMM0_DDR2_A0" LOC ="AA42";
NET "DBG_LED_3" LOC ="AL6";
NET "DBG_LED_2" LOC ="AN5";
NET "DBG_LED_1" LOC ="AP6";
NET "DBG_LED_0" LOC ="AL7";
NET "CPU_TRST_B" LOC ="AT30";
NET "CPU_TMS" LOC ="AR14";
NET "CPU_TDO_TMP" LOC ="AR28";
NET "CPU_TDI" LOC ="AR30";
NET "CPU_TCK" LOC ="AT14";
NET "CPU_HALT_B" LOC ="AR29";
NET "ATD_4" LOC ="AM24";
NET "ATD_3" LOC ="AT19";
NET "ATD_2" LOC ="AP25";
NET "ATD_1" LOC ="AN25";
NET "ATD_0" LOC ="AP26";
NET "ATCB_CLK_R" LOC ="J16";
NET "$3N7315" LOC ="R30";
NET "$3N7288" LOC ="AF30";
NET "$3N7283" LOC ="T30";
