ADDRESS_ACLR_A=NONE
CLOCK_ENABLE_INPUT_A=BYPASS
CLOCK_ENABLE_OUTPUT_A=BYPASS
INIT_FILE=progmem.mif
INTENDED_DEVICE_FAMILY="Cyclone IV GX"
MAXIMUM_DEPTH=8192
NUMWORDS_A=65536
OPERATION_MODE=ROM
OUTDATA_ACLR_A=NONE
OUTDATA_REG_A=UNREGISTERED
WIDTHAD_A=16
WIDTH_A=32
WIDTH_BYTEENA_A=1
DEVICE_FAMILY="Cyclone IV GX"
address_a
clock0
q_a
