Function Index
$#! · 0-9 · A · B · C · D · E · F · G · H · I · J · K · L · M · N · O · P · Q · R · S · T · U · V · W · X · Y · Z

C |
| cmp_complex
| cmp_idx
| core_bench_matrix
| core_bench_state
| core_init_state
| core_list_find
| core_list_init
| core_list_insert
| core_list_mergesort
| core_list_remove
| core_list_reverse
| core_list_undo_remove
| core_start_parallel
| core_state_transition
| core_stop_parallel
| crc*
G |
| get_seed
| get_time
I |
| iterate
M |
| main
| matrix_add_const
| matrix_mul_const
| matrix_mul_matrix
| matrix_mul_matrix_bitextract
| matrix_mul_vect
| matrix_sum
| matrix_test
P |
| portable_fini
| portable_free
| portable_init
| portable_malloc
S |
| start_time
| stop_time
T |
| time_in_secs

> ee_s32 cmp_complex( | list_data | * | a,
> | list_data | * | b,
> | core_results | * | res | )

Compare the data item in a list cell.

> ee_s32 cmp_idx( | list_data | * | a,
> | list_data | * | b,
> | core_results | * | res | )

Compare the idx item in a list cell, and regen the data.

> ee_u16 core_bench_matrix( | mat_params | * | p,
> | ee_s16 |  | seed,
> | ee_u16 |  | crc | )

Benchmark function

> ee_u16 core_bench_state( | ee_u32 |  | blksize,
> | ee_u8 | * | memblock,
> | ee_s16 |  | seed1,
> | ee_s16 |  | seed2,
> | ee_s16 |  | step,
> | ee_u16 |  | crc | )

Benchmark function

> void core_init_state( | ee_u32 |  | size,
> | ee_s16 |  | seed,
> | ee_u8 | * | p | )

Initialize the input data for the state machine.

> list_head *core_list_find( | list_head | * | list,
> | list_data | * | info | )

Find an item in the list

> list_head *core_list_init( | ee_u32 |  | blksize,
> | list_head | * | memblock,
> | ee_s16 |  | seed | )

Initialize list with data.

> list_head *core_list_insert_new( |  | list_head | * | insert_point,
> |  | list_data | * | info,
> |  | list_head | ** | memblock,
> | list_data | **datablock |  | ,
> |  | list_head | * | memblock_end,
> |  | list_data | * | datablock_end | )

Insert an item to the list

> list_head *core_list_mergesort( | list_head | * | list,
> | list_cmp |  | cmp,
> | core_results | * | res | )

Sort the list in place without recursion.

> list_head *core_list_remove( | list_head | * | item | )

Remove an item from the list.

> list_head *core_list_reverse( | list_head | * | list | )

Reverse a list

> list_head *core_list_undo_remove( | list_head | * | item_removed,
> | list_head | * | item_modified | )

Undo a remove operation.
Start benchmarking in a parallel context.

> enum CORE_STATE core_state_transition( | ee_u8 | **instr |  | ,
> |  | ee_u32 | * | transition_count | )

Actual state machine.
Stop a parallel context execution of coremark, and gather the results.
Service functions to calculate 16b CRC code.
Get a values that cannot be determined at compile time.

> CORE_TICKS get_time( | void | )

Return an abstract “ticks” number that signifies time on the system.
Run the benchmark for a specified number of iterations.

> #if MAIN_HAS_NOARGC MAIN_RETURN_TYPE main( | void | )

Main entry routine for the benchmark.

> void matrix_add_const( | ee_u32 |  | N,
> | MATDAT | * | A,
> | MATDAT |  | val | )

Add a constant value to all elements of a matrix.

> void matrix_mul_const( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT | * | A,
> | MATDAT |  | val | )

Multiply a matrix by a constant.

> void matrix_mul_matrix( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT | * | A,
> | MATDAT | * | B | )

Multiply a matrix by a matrix.

> void matrix_mul_matrix_bitextract( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT | * | A,
> | MATDAT | * | B | )

Multiply a matrix by a matrix, and extract some bits from the result.

> void matrix_mul_vect( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT | * | A,
> | MATDAT | * | B | )

Multiply a matrix by a vector.

> ee_s16 matrix_sum( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT |  | clipval | )

Calculate a function that depends on the values of elements in the matrix.

> ee_s16 matrix_test( | ee_u32 |  | N,
> | MATRES | * | C,
> | MATDAT | * | A,
> | MATDAT | * | B,
> | MATDAT |  | val | )

Perform matrix manipulation.

> void portable_fini( | core_portable | * | p | )

Target specific final code

> void portable_free( | void | * | p | )

Provide free() functionality in a platform specific way.

> void portable_init( | core_portable | * | p,
> | int | * | argc,
> | char | * | argv[] | )

Target specific initialization code Test for some common mistakes.

> void *portable_malloc( | size_t | size | )

Provide malloc() functionality in a platform specific way.

> void start_time( | void | )

This function will be called right before starting the timed portion of the benchmark.

> void stop_time( | void | )

This function will be called right after ending the timed portion of the benchmark.

> secs_ret time_in_secs( | CORE_TICKS | ticks | )

Convert the value returned by get_time to seconds.
Close